AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
SPI_for_AFE Member List

This is the complete list of members for SPI_for_AFE, including all inherited members.

burst(uint32_t *data, int length, int width=3) | SPI_for_AFE |
command_length | SPI_for_AFE | private static
get_data16(uint8_t *vp) | SPI_for_AFE | inline private
get_data24(uint8_t *vp) | SPI_for_AFE | inline private
init(void) | SPI_for_AFE | protected
read_r16(uint16_t reg) | SPI_for_AFE |
read_r24(uint16_t reg) | SPI_for_AFE |
txrx(uint8_t *data, int size) | SPI_for_AFE |
write_r16(uint16_t reg) | SPI_for_AFE |
write_r16(uint16_t reg, uint16_t val) | SPI_for_AFE |
write_r24(uint16_t reg, uint32_t val) | SPI_for_AFE |