AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Classes | Functions
NAFE33352.h File Reference
`#include <Arduino.h>`
`#include "AFE_NXP.h"`
`#include "SPI_for_AFE.h"`

Go to the source code of this file.

## Classes
class | NAFE33352_Base
class | NAFE33352_Base::LogicalChannel
class | NAFE33352_Base::DAC
class | NAFE33352
class | NAFE33352_UIOM

## Functions
NAFE33352_Base::Register16 | operator+ (NAFE33352_Base::Register16 rn, int n)
NAFE33352_Base::Register16 | operator+ (int n, NAFE33352_Base::Register16 rn)
NAFE33352_Base::Register24 | operator+ (NAFE33352_Base::Register24 rn, int n)
NAFE33352_Base::Register24 | operator+ (int n, NAFE33352_Base::Register24 rn)

## Function Documentation

## ◆ operator+() [1/4]

NAFE33352_Base::Register16 operator+ | ( | int | n,
|  | NAFE33352_Base::Register16 | rn )
| inline

Definition at line 498 of file NAFE33352.h.

## ◆ operator+() [2/4]

NAFE33352_Base::Register24 operator+ | ( | int | n,
|  | NAFE33352_Base::Register24 | rn )
| inline

Definition at line 508 of file NAFE33352.h.

## ◆ operator+() [3/4]

NAFE33352_Base::Register16 operator+ | ( | NAFE33352_Base::Register16 | rn,
|  | int | n )
| inline

Definition at line 493 of file NAFE33352.h.

## ◆ operator+() [4/4]

NAFE33352_Base::Register24 operator+ | ( | NAFE33352_Base::Register24 | rn,
|  | int | n )
| inline

Definition at line 503 of file NAFE33352.h.