AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all variables with links to the classes they belong to:

### - a -

- afe_ptr : LogicalChannel_Base, NAFE33352_Base::DAC

### - c -

- cal_index : NAFE13388_Base::_ref_points
- cbf_DRDY : AFE_base
- ch_delay : AFE_base
- ch_number : LogicalChannel_Base
- coeff_index : NAFE13388_Base::_ref_points
- coeff_V : AFE_base
- command_length : SPI_for_AFE

### - d -

- dac : NAFE33352_Base
- data : NAFE13388_Base::_reference_point
- delay_accuracy : AFE_base
- dev_add : AFE_base
- drdy_count : AFE_base
- drdy_flag : AFE_base

### - e -

- enabled_channels : AFE_base

### - f -

- full_scale : NAFE33352_Base::DAC

### - h -

- high : NAFE13388_Base::_ref_points
- highspeed_variant : AFE_base

### - i -

- instance : AFE_base

### - l -

- logical_channel : NAFE13388_Base, NAFE33352_Base
- low : NAFE13388_Base::_ref_points

### - m -

- mux_setting : AFE_base

### - o -

- on_board_shunt_resister : NAFE33352_Base
- output_mode : NAFE33352_Base::DAC

### - p -

- pga_gain : NAFE13388_Base, NAFE33352_Base
- pin_DRDY : AFE_base
- pin_DRDY_input : AFE_base
- pin_nINT : AFE_base
- pin_nRESET : AFE_base
- pin_SYN : AFE_base
- pin_SYNCDAC : AFE_base

### - s -

- sequence_order : AFE_base

### - t -

- timeout_limit : AFE_base
- total_delay : AFE_base

### - v -

- voltage : NAFE13388_Base::_reference_point