AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Public Member Functions | List of all members
NAFE13388 Class Reference

`#include <AFE_NXP.h>`

Inheritance diagram for NAFE13388:

## Public Member Functions
| NAFE13388 (bool spi_addr=0, bool highspeed_variant=false, int nINT=2, int DRDY=4, int SYN=5, int nRESET=6, int DRDY_input=15, int SYNCDAC=14)
virtual | ~NAFE13388 ()
Public Member Functions inherited from NAFE13388_Base
| NAFE13388_Base (bool spi_addr, bool highspeed_variant, int nINT, int DRDY, int SYN, int nRESET, int DRDY_input, int SYNCDAC)
virtual | ~NAFE13388_Base ()
virtual void | boot (void)
virtual void | reset (bool hardware_reset=false)
virtual void | open_logical_channel (int ch, uint16_t cc0, uint16_t cc1, uint16_t cc2, uint16_t cc3)
virtual void | open_logical_channel (int ch, const uint16_t(&cc)[4])
virtual void | close_logical_channel (int ch)
virtual void | close_logical_channel (void)
void | enable_logical_channel (int ch)
virtual void | start (int ch)
virtual void | start (void)
virtual void | start_continuous_conversion ()
virtual void | DRDY_by_sequencer_done (bool flag=true)
virtual raw_t | read (int ch)
virtual void | read (raw_t *data)
virtual void | read (volt_t *data)
double | raw2v (int ch, raw_t value)
virtual void | command (uint16_t com)
virtual void | reg (Register16 r, uint16_t value)
virtual void | reg (Register24 r, uint32_t value)
virtual uint16_t | reg (Register16 r)
virtual uint32_t | reg (Register24 r)
template<typename T>
uint32_t | bit_op (T rg, uint32_t mask, uint32_t value)
uint32_t | part_number (void)
uint8_t | revision_number (void)
uint64_t | serial_number (void)
float | temperature (void)
void | gain_offset_coeff (const ref_points &ref)
int | self_calibrate (int pga_gain_index, int channel_selection=15, int input_select=0, double reference_source_voltage=0, bool use_positive_side=true)
void | blink_leds (void)
Public Member Functions inherited from AFE_base
| AFE_base (bool spi_addr, bool highspeed_variant, int nINT, int DRDY, int SYN, int nRESET, int DRDY_input, int SYNCDAC)
virtual | ~AFE_base ()
virtual void | begin (void)
virtual void | set_DRDY_callback (callback_fp_t fnc)
virtual raw_t | start_and_read (int ch)
template<typename T>
void | start_and_read (T data)
double | raw2uv (int ch, raw_t value)
double | raw2mv (int ch, raw_t value)
double | drdy_delay (int ch)
double | drdy_delay (void)
int | enabled_logical_channels (void)
void | use_DRDY_trigger (bool use=true)
Public Member Functions inherited from SPI_for_AFE
void | txrx (uint8_t *data, int size)
void | write_r16 (uint16_t reg)
void | write_r16 (uint16_t reg, uint16_t val)
uint16_t | read_r16 (uint16_t reg)
void | write_r24 (uint16_t reg, uint32_t val)
int32_t | read_r24 (uint16_t reg)
void | burst (uint32_t *data, int length, int width=3)

## Additional Inherited Members
Public Types inherited from NAFE13388_Base
enum | GainPGA : uint8_t { G_PGA_x_0_2 = 0 , G_PGA_x_0_4 , G_PGA_x_0_8 , G_PGA_x_1_0 , G_PGA_x_2_0 , G_PGA_x_4_0 , G_PGA_x_8_0 , G_PGA_x16_0 }
enum class | Register16 : uint16_t { CH_CONFIG0 = 0x20 , CH_CONFIG1 = 0x21 , CH_CONFIG2 = 0x22 , CH_CONFIG3 = 0x23 , CH_CONFIG4 = 0x24 , CRC_CONF_REGS = 0x25 , CRC_COEF_REGS = 0x26 , CRC_TRIM_REGS = 0x27 , GPI_DATA = 0x29 , GPIO_CONFIG0 = 0x2A , GPIO_CONFIG1 = 0x2B , GPIO_CONFIG2 = 0x2C , GPI_EDGE_POS = 0x2D , GPI_EDGE_NEG = 0x2E , GPO_DATA = 0x2F , SYS_CONFIG0 = 0x30 , SYS_STATUS0 = 0x31 , GLOBAL_ALARM_ENABLE = 0x32 , GLOBAL_ALARM_INTERRUPT = 0x33 , DIE_TEMP = 0x34 , CH_STATUS0 = 0x35 , CH_STATUS1 = 0x36 , THRS_TEMP = 0x37 , PN2 = 0x7C , PN1 = 0x7D , PN0 = 0x7E , CRC_TRIM_INT = 0x7F }
enum class | Register24 : uint16_t { CH_DATA0 = 0x40 , CH_DATA1 = 0x41 , CH_DATA2 = 0x42 , CH_DATA3 = 0x43 , CH_DATA4 = 0x44 , CH_DATA5 = 0x45 , CH_DATA6 = 0x46 , CH_DATA7 = 0x47 , CH_DATA8 = 0x48 , CH_DATA9 = 0x4A , CH_DATA10 = 0x4B , CH_DATA11 = 0x4C , CH_DATA13 = 0x4D , CH_DATA14 = 0x4E , CH_DATA15 = 0x4F , CH_CONFIG5_0 = 0x50 , CH_CONFIG5_1 = 0x51 , CH_CONFIG5_2 = 0x52 , CH_CONFIG5_3 = 0x53 , CH_CONFIG5_4 = 0x54 , CH_CONFIG5_5 = 0x55 , CH_CONFIG5_6 = 0x56 , CH_CONFIG5_7 = 0x57 , CH_CONFIG5_8 = 0x58 , CH_CONFIG5_9 = 0x59 , CH_CONFIG5_10 = 0x5A , CH_CONFIG5_11 = 0x5B , CH_CONFIG5_12 = 0x5C , CH_CONFIG5_13 = 0x5D , CH_CONFIG5_14 = 0x5E , CH_CONFIG5_15 = 0x5F , CH_CONFIG6_0 = 0x60 , CH_CONFIG6_1 = 0x61 , CH_CONFIG6_2 = 0x62 , CH_CONFIG6_3 = 0x63 , CH_CONFIG6_4 = 0x64 , CH_CONFIG6_5 = 0x65 , CH_CONFIG6_6 = 0x66 , CH_CONFIG6_7 = 0x67 , CH_CONFIG6_8 = 0x68 , CH_CONFIG6_9 = 0x69 , CH_CONFIG6_10 = 0x6A , CH_CONFIG6_11 = 0x6B , CH_CONFIG6_12 = 0x6C , CH_CONFIG6_13 = 0x6D , CH_CONFIG6_14 = 0x6E , CH_CONFIG6_15 = 0x6F , GAIN_COEFF0 = 0x80 , GAIN_COEFF1 = 0x81 , GAIN_COEFF2 = 0x82 , GAIN_COEFF3 = 0x83 , GAIN_COEFF4 = 0x84 , GAIN_COEFF5 = 0x85 , GAIN_COEFF6 = 0x86 , GAIN_COEFF7 = 0x87 , GAIN_COEFF8 = 0x88 , GAIN_COEFF9 = 0x89 , GAIN_COEFF10 = 0x8A , GAIN_COEFF11 = 0x8B , GAIN_COEFF12 = 0x8C , GAIN_COEFF13 = 0x8D , GAIN_COEFF14 = 0x8E , GAIN_COEFF15 = 0x8F , OFFSET_COEFF0 = 0x90 , OFFSET_COEFF1 = 0x91 , OFFSET_COEFF2 = 0x92 , OFFSET_COEFF3 = 0x93 , OFFSET_COEFF4 = 0x94 , OFFSET_COEFF5 = 0x95 , OFFSET_COEFF6 = 0x96 , OFFSET_COEFF7 = 0x97 , OFFSET_COEFF8 = 0x98 , OFFSET_COEFF9 = 0x99 , OFFSET_COEFF10 = 0x9A , OFFSET_COEFF11 = 0x9B , OFFSET_COEFF12 = 0x9C , OFFSET_COEFF13 = 0x9D , OFFSET_COEFF14 = 0x9E , OFFSET_COEFF15 = 0x9F , OPT_COEF0 = 0xA0 , OPT_COEF1 = 0xA1 , OPT_COEF2 = 0xA2 , OPT_COEF3 = 0xA3 , OPT_COEF4 = 0xA4 , OPT_COEF5 = 0xA5 , OPT_COEF6 = 0xA6 , OPT_COEF7 = 0xA7 , OPT_COEF8 = 0xA8 , OPT_COEF9 = 0xA9 , OPT_COEF10 = 0xAA , OPT_COEF11 = 0xAB , OPT_COEF12 = 0xAC , OPT_COEF13 = 0xAD , SERIAL1 = 0xAE , SERIAL0 = 0xAF }
enum | Command : uint16_t { CMD_CH0 = 0x0000 , CMD_CH1 = 0x0001 , CMD_CH2 = 0x0002 , CMD_CH3 = 0x0003 , CMD_CH4 = 0x0004 , CMD_CH5 = 0x0005 , CMD_CH6 = 0x0006 , CMD_CH7 = 0x0007 , CMD_CH8 = 0x0008 , CMD_CH9 = 0x0009 , CMD_CH10 = 0x000A , CMD_CH11 = 0x000B , CMD_CH12 = 0x000C , CMD_CH13 = 0x000D , CMD_CH14 = 0x000E , CMD_CH15 = 0x000F , CMD_ABORT = 0x0010 , CMD_END = 0x0011 , CMD_CLEAR_ALARM = 0x0012 , CMD_CLEAR_DATA = 0x0013 , CMD_RESET = 0x0014 , CMD_CLEAR_REG = 0x0015 , CMD_RELOAD = 0x0016 , TBD = 0x0017 , CMD_SS = 0x2000 , CMD_SC = 0x2001 , CMD_MM = 0x2002 , CMD_MC = 0x2003 , CMD_MS = 0x2004 , CMD_BURST_DATA = 0x2005 , CMD_CALC_CRC_CONFG = 0x2006 , CMD_CALC_CRC_COEF = 0x2007 , CMD_CALC_CRC_FAC = 0x2008 }
enum | CalibrationError : int { NoError = 0 , GainError = -1 , OffsetError = -2 }
using | ch_setting_t = uint16_t[ 4 ]
typedef struct NAFE13388_Base::_reference_point | reference_point
typedef struct NAFE13388_Base::_ref_points | ref_points
Public Types inherited from AFE_base
enum | LV_mux_sel : uint8_t { REF2_REF2 = 0 , GPIO0_GPIO1 , REFCOARSE_REF2 , VADD_REF2 , VHDD_REF2 , REF2_VHSS , HV_MUX }
using | raw_t = int32_t
using | volt_t = double
typedef void(* | callback_fp_t) (void)
Public Attributes inherited from NAFE13388_Base
LogicalChannel | logical_channel [16]
Static Public Attributes inherited from NAFE13388_Base
static double | pga_gain [] = { 0.2, 0.4, 0.8, 1, 2, 4, 8, 16 }
Static Public Attributes inherited from AFE_base
static AFE_base * | instance = nullptr
Protected Member Functions inherited from AFE_base
int | bit_count (uint32_t value)
void | default_drdy_cb ()
virtual void | init (void)
int | wait_conversion_complete (double delay=-1.0)
Protected Member Functions inherited from SPI_for_AFE
void | init (void)
Static Protected Member Functions inherited from AFE_base
static void | static_default_drdy_cb ()
static void | DRDY_cb ()
Protected Attributes inherited from AFE_base
bool | dev_add
bool | highspeed_variant
int | pin_nINT
int | pin_DRDY
int | pin_SYN
int | pin_nRESET
int | pin_DRDY_input
int | pin_SYNCDAC
int | enabled_channels
uint8_t | sequence_order [16]
double | coeff_V [16]
int | mux_setting [16]
double | ch_delay [16]
double | total_delay
uint32_t | drdy_count
volatile bool | drdy_flag
Static Protected Attributes inherited from AFE_base
static double | delay_accuracy = 1.1
static constexpr uint32_t | timeout_limit = 10000000
static callback_fp_t | cbf_DRDY = nullptr

## Detailed Description

Definition at line 726 of file AFE_NXP.h.

## Constructor & Destructor Documentation

## ◆ NAFE13388()

NAFE13388::NAFE13388 | ( | bool | spi_addr = 0,
|  | bool | highspeed_variant = false,
|  | int | nINT = 2,
|  | int | DRDY = 4,
|  | int | SYN = 5,
|  | int | nRESET = 6,
|  | int | DRDY_input = 15,
|  | int | SYNCDAC = 14 )

Constructor to create a NAFE13388 instance

Definition at line 615 of file AFE_NXP.cpp.

## ◆ ~NAFE13388()

NAFE13388::~NAFE13388 | ( |  | ) |
| virtual

Destractor

Definition at line 620 of file AFE_NXP.cpp.

The documentation for this class was generated from the following files:

- AFE_NXP.h
- AFE_NXP.cpp