AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - r -

- raw2mv() : AFE_base
- raw2uv() : AFE_base
- raw2v() : AFE_base, NAFE13388_Base, NAFE33352_Base
- raw_t : AFE_base
- read() : AFE_base, LogicalChannel_Base, NAFE13388_Base, NAFE33352_Base
- read_r16() : SPI_for_AFE
- read_r24() : SPI_for_AFE
- REF2_REF2 : AFE_base
- REF2_VHSS : AFE_base
- REF_BYP__VCM : NAFE33352_Base
- ref_points : NAFE13388_Base
- REFCOARSE_REF2 : AFE_base
- reference_point : NAFE13388_Base
- reg() : NAFE13388_Base, NAFE33352_Base
- Register16 : NAFE13388_Base, NAFE33352_Base
- Register24 : NAFE13388_Base, NAFE33352_Base
- reset() : AFE_base, NAFE13388_Base, NAFE33352_Base
- revision_number() : NAFE13388_Base, NAFE33352_Base