AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all functions with links to the classes they belong to:

### - a -

- AFE_base() : AFE_base

### - b -

- begin() : AFE_base
- bit_count() : AFE_base
- bit_op() : NAFE13388_Base, NAFE33352_Base
- blink_leds() : NAFE13388_Base, NAFE13388_UIM
- boot() : AFE_base, NAFE13388_Base, NAFE33352_Base
- burst() : SPI_for_AFE

### - c -

- calc_delay() : NAFE13388_Base, NAFE33352_Base
- channel_info_update() : NAFE13388_Base, NAFE33352_Base
- close_logical_channel() : AFE_base, NAFE13388_Base, NAFE33352_Base
- command() : NAFE13388_Base, NAFE33352_Base
- configure() : NAFE13388_Base::LogicalChannel, NAFE33352_Base::DAC, NAFE33352_Base::LogicalChannel

### - d -

- DAC() : NAFE33352_Base::DAC
- dac_code() : NAFE33352_Base
- dac_out() : NAFE33352_Base
- default_drdy_cb() : AFE_base
- disable() : LogicalChannel_Base
- DRDY_by_sequencer_done() : AFE_base, NAFE13388_Base, NAFE33352_Base
- DRDY_cb() : AFE_base
- drdy_delay() : AFE_base

### - e -

- enable() : LogicalChannel_Base
- enable_logical_channel() : AFE_base, NAFE13388_Base, NAFE33352_Base
- enabled_logical_channels() : AFE_base

### - g -

- gain_offset_coeff() : NAFE13388_Base
- get_data16() : SPI_for_AFE
- get_data24() : SPI_for_AFE

### - i -

- init() : AFE_base, SPI_for_AFE

### - l -

- LogicalChannel() : NAFE13388_Base::LogicalChannel, NAFE33352_Base::LogicalChannel
- LogicalChannel_Base() : LogicalChannel_Base

### - n -

- NAFE13388() : NAFE13388
- NAFE13388_Base() : NAFE13388_Base
- NAFE13388_UIM() : NAFE13388_UIM
- NAFE33352() : NAFE33352
- NAFE33352_Base() : NAFE33352_Base
- NAFE33352_UIOM() : NAFE33352_UIOM

### - o -

- open_dac_output() : NAFE33352_Base
- open_logical_channel() : AFE_base, NAFE13388_Base, NAFE33352_Base
- operator AFE_base::raw_t() : LogicalChannel_Base
- operator AFE_base::volt_t() : LogicalChannel_Base
- operator*() : LogicalChannel_Base
- operator+() : LogicalChannel_Base
- operator-() : LogicalChannel_Base
- operator/() : LogicalChannel_Base
- operator=() : NAFE33352_Base::DAC
- output() : NAFE33352_Base::DAC

### - p -

- part_number() : NAFE13388_Base, NAFE33352_Base

### - r -

- raw2mv() : AFE_base
- raw2uv() : AFE_base
- raw2v() : AFE_base, NAFE13388_Base, NAFE33352_Base
- read() : AFE_base, LogicalChannel_Base, NAFE13388_Base, NAFE33352_Base
- read_r16() : SPI_for_AFE
- read_r24() : SPI_for_AFE
- reg() : NAFE13388_Base, NAFE33352_Base
- reset() : AFE_base, NAFE13388_Base, NAFE33352_Base
- revision_number() : NAFE13388_Base, NAFE33352_Base

### - s -

- self_calibrate() : NAFE13388_Base
- serial_number() : NAFE13388_Base, NAFE33352_Base
- set_DRDY_callback() : AFE_base
- start() : AFE_base, NAFE13388_Base, NAFE33352_Base
- start_and_read() : AFE_base
- start_continuous_conversion() : AFE_base, NAFE13388_Base, NAFE33352_Base
- static_default_drdy_cb() : AFE_base

### - t -

- temperature() : NAFE13388_Base, NAFE33352_Base
- txrx() : SPI_for_AFE

### - u -

- use_DRDY_trigger() : AFE_base

### - w -

- wait_conversion_complete() : AFE_base
- write_r16() : SPI_for_AFE
- write_r24() : SPI_for_AFE

### - ~ -

- ~AFE_base() : AFE_base
- ~DAC() : NAFE33352_Base::DAC
- ~LogicalChannel() : NAFE13388_Base::LogicalChannel, NAFE33352_Base::LogicalChannel
- ~LogicalChannel_Base() : LogicalChannel_Base
- ~NAFE13388() : NAFE13388
- ~NAFE13388_Base() : NAFE13388_Base
- ~NAFE13388_UIM() : NAFE13388_UIM
- ~NAFE33352() : NAFE33352
- ~NAFE33352_Base() : NAFE33352_Base
- ~NAFE33352_UIOM() : NAFE33352_UIOM