AFE_NXP_Arduino 2.0.2 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
NAFE33352_Base::DAC Member List

This is the complete list of members for NAFE33352_Base::DAC, including all inherited members.

afe_ptr | NAFE33352_Base::DAC |
configure(const uint16_t(&cc)[6]) | NAFE33352_Base::DAC |
configure(uint16_t cc0, uint16_t cc1, uint16_t cc2, uint16_t cc3, uint16_t cc4, uint16_t cc5) | NAFE33352_Base::DAC |
configure(ModeSelect mode, double full_scale_range=0.00) | NAFE33352_Base::DAC |
configure(double full_scale_range) | NAFE33352_Base::DAC |
DAC() | NAFE33352_Base::DAC |
full_scale | NAFE33352_Base::DAC | private
ModeSelect enum name | NAFE33352_Base::DAC |
operator=(double value) | NAFE33352_Base::DAC |
output(double value) | NAFE33352_Base::DAC |
output_mode | NAFE33352_Base::DAC | private
~DAC() | NAFE33352_Base::DAC | virtual