AFE_NXP_Arduino 1.0.3 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
5_0_NAFE13388_RTD_4_wire Directory Reference

## Detailed Description

# 5_0_NAFE13388_RTD_4_wire

Practical sample to measure temperature by 2 RTDs using internal current excitation source.
These RTD measurements are done in 4 wire method.

This sample uses 2 logical channels for each RTDs.
The logical channel setting defines analog input channel selections as well as excitation current configurations.

# Wiring

# Logical channel setting on channel 0

# Logical channel setting on channel 1