AFE_NXP_Arduino 2.0.4 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:
A
B
C
D
E
F
G
H
I
L
M
N
O
P
R
S
T
U
V
W
~

### - c -

- cal_index : NAFE13388_Base::_ref_points
- calc_delay() : NAFE13388_Base, NAFE33352_Base
- CalibrationError : NAFE13388_Base
- callback_fp_t : AFE_base
- cbf_DRDY : AFE_base
- ch_delay : AFE_base
- ch_number : LogicalChannel_Base
- ch_setting_t : NAFE13388_Base, NAFE33352_Base
- channel_info_update() : NAFE13388_Base, NAFE33352_Base
- close_logical_channel() : AFE_base, NAFE13388_Base, NAFE33352_Base
- CMD_ABORT : NAFE13388_Base
- CMD_ADC_ABORT : NAFE33352_Base
- CMD_AO_ABORT : NAFE33352_Base
- CMD_AO_ABORT_HIZ : NAFE33352_Base
- CMD_BURST_DATA : NAFE13388_Base, NAFE33352_Base
- CMD_CALC_CRC_COEF : NAFE13388_Base, NAFE33352_Base
- CMD_CALC_CRC_CONFG : NAFE13388_Base
- CMD_CALC_CRC_CONFIG : NAFE33352_Base
- CMD_CALC_CRC_FAC : NAFE13388_Base, NAFE33352_Base
- CMD_CH0 : NAFE13388_Base, NAFE33352_Base
- CMD_CH1 : NAFE13388_Base, NAFE33352_Base
- CMD_CH10 : NAFE13388_Base
- CMD_CH11 : NAFE13388_Base
- CMD_CH12 : NAFE13388_Base
- CMD_CH13 : NAFE13388_Base
- CMD_CH14 : NAFE13388_Base
- CMD_CH15 : NAFE13388_Base
- CMD_CH2 : NAFE13388_Base, NAFE33352_Base
- CMD_CH3 : NAFE13388_Base, NAFE33352_Base
- CMD_CH4 : NAFE13388_Base, NAFE33352_Base
- CMD_CH5 : NAFE13388_Base, NAFE33352_Base
- CMD_CH6 : NAFE13388_Base, NAFE33352_Base
- CMD_CH7 : NAFE13388_Base, NAFE33352_Base
- CMD_CH8 : NAFE13388_Base
- CMD_CH9 : NAFE13388_Base
- CMD_CISW_ABORT : NAFE33352_Base
- CMD_CISW_ABORT_HIZ : NAFE33352_Base
- CMD_CLEAR_ALARM : NAFE13388_Base, NAFE33352_Base
- CMD_CLEAR_DAC0 : NAFE33352_Base
- CMD_CLEAR_DATA : NAFE13388_Base, NAFE33352_Base
- CMD_CLEAR_REG : NAFE13388_Base, NAFE33352_Base
- CMD_END : NAFE13388_Base, NAFE33352_Base
- CMD_MC : NAFE13388_Base, NAFE33352_Base
- CMD_MM : NAFE13388_Base, NAFE33352_Base
- CMD_MS : NAFE13388_Base, NAFE33352_Base
- CMD_RELOAD : NAFE13388_Base, NAFE33352_Base
- CMD_RESET : NAFE13388_Base, NAFE33352_Base
- CMD_SC : NAFE13388_Base, NAFE33352_Base
- CMD_SS : NAFE13388_Base, NAFE33352_Base
- CMD_WGEN_START : NAFE33352_Base
- CMD_WGEN_STOP : NAFE33352_Base
- coeff_index : NAFE13388_Base::_ref_points
- coeff_V : AFE_base
- Command : NAFE13388_Base, NAFE33352_Base
- command() : NAFE13388_Base, NAFE33352_Base
- command_length : SPI_for_AFE
- configure() : NAFE13388_Base::LogicalChannel, NAFE33352_Base::DAC, NAFE33352_Base::LogicalChannel