# 6_0_NAFE13388_Thermocouple

Practical sample to measure temperature by thermocouple with on-board RTD.  
The thermocouple measured temperature is conpensated by RTD on GPIO0-GPIO1 pins.  

This sample uses 2 logical channels for thermocouple and RTD.  

## Wiring
![](img/conection_TC.png)

## Logical channel setting on channel 0

![](img/logical_channel_setting_ch0.png)

## Logical channel setting on channel 1

![](img/logical_channel_setting_ch1.png)
