AFE_NXP_Arduino 2.0.4 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
NAFE13388_6_0_Thermocouple Directory Reference

## Detailed Description

# 6_0_NAFE13388_Thermocouple

Practical sample to measure temperature by thermocouple with on-board RTD.
The thermocouple measured temperature is conpensated by RTD on GPIO0-GPIO1 pins.

This sample uses 2 logical channels for thermocouple and RTD.

# Wiring

# Logical channel setting on channel 0

# Logical channel setting on channel 1