AFE_NXP_Arduino 2.0.5 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Here is a list of all class members with links to the classes they belong to:

### - g -

- G_PGA_x16_0 : NAFE13388_Base, NAFE33352_Base
- G_PGA_x_0_2 : NAFE13388_Base
- G_PGA_x_0_4 : NAFE13388_Base
- G_PGA_x_0_8 : NAFE13388_Base
- G_PGA_x_1_0 : NAFE13388_Base, NAFE33352_Base
- G_PGA_x_2_0 : NAFE13388_Base
- G_PGA_x_4_0 : NAFE13388_Base
- G_PGA_x_8_0 : NAFE13388_Base
- gain_offset_coeff() : NAFE13388_Base
- GainError : NAFE13388_Base
- GainPGA : NAFE13388_Base, NAFE33352_Base
- get_data16() : SPI_for_AFE
- get_data24() : SPI_for_AFE
- GPIO0_GPIO1 : AFE_base, NAFE33352_Base
- GPIO0_VCM : NAFE33352_Base