AFE_NXP_Arduino 2.0.5 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
Classes | Functions
AFE_NXP.h File Reference
`#include <Arduino.h>`
`#include <math.h>`
`#include <stdint.h>`
`#include <SPI_for_AFE.h>`

Go to the source code of this file.

## Classes
class | AFE_base
class | LogicalChannel_Base
class | NAFE13388_Base
struct | NAFE13388_Base::_reference_point
struct | NAFE13388_Base::_ref_points
class | NAFE13388_Base::LogicalChannel
class | NAFE13388
class | NAFE13388_UIM

## Functions
NAFE13388_Base::Register16 | operator+ (NAFE13388_Base::Register16 rn, int n)
NAFE13388_Base::Register16 | operator+ (int n, NAFE13388_Base::Register16 rn)
NAFE13388_Base::Register24 | operator+ (NAFE13388_Base::Register24 rn, int n)
NAFE13388_Base::Register24 | operator+ (int n, NAFE13388_Base::Register24 rn)

## Function Documentation

## ◆ operator+() [1/4]

NAFE13388_Base::Register16 operator+ | ( | int | n,
|  | NAFE13388_Base::Register16 | rn
| ) |  |
| inline

Definition at line 797 of file AFE_NXP.h.

## ◆ operator+() [2/4]

NAFE13388_Base::Register24 operator+ | ( | int | n,
|  | NAFE13388_Base::Register24 | rn
| ) |  |
| inline

Definition at line 807 of file AFE_NXP.h.

## ◆ operator+() [3/4]

NAFE13388_Base::Register16 operator+ | ( | NAFE13388_Base::Register16 | rn,
|  | int | n
| ) |  |
| inline

Definition at line 792 of file AFE_NXP.h.

## ◆ operator+() [4/4]

NAFE13388_Base::Register24 operator+ | ( | NAFE13388_Base::Register24 | rn,
|  | int | n
| ) |  |
| inline

Definition at line 802 of file AFE_NXP.h.