AFE_NXP_Arduino 2.0.5 Analog Front-End (AFE) device operation sample code for Arduino

Loading...
Searching...
No Matches
NAFE33352_Base::LogicalChannel Member List

This is the complete list of members for NAFE33352_Base::LogicalChannel, including all inherited members.

afe_ptr | LogicalChannel_Base |
ch_number | LogicalChannel_Base |
configure(const uint16_t(&cc)[3]) | NAFE33352_Base::LogicalChannel |
configure(uint16_t cc0, uint16_t cc1=0x0000, uint16_t cc2=0x0000) | NAFE33352_Base::LogicalChannel |
disable(void) | LogicalChannel_Base |
enable(void) | LogicalChannel_Base |
LogicalChannel() | NAFE33352_Base::LogicalChannel |
LogicalChannel_Base() | LogicalChannel_Base | inline
operator AFE_base::raw_t(void) | LogicalChannel_Base |
operator AFE_base::volt_t(void) | LogicalChannel_Base |
operator*(T v) | LogicalChannel_Base | inline
operator+(T v) | LogicalChannel_Base | inline
operator-(T v) | LogicalChannel_Base | inline
operator/(T v) | LogicalChannel_Base | inline
read(void) | LogicalChannel_Base |
read(void) | LogicalChannel_Base |
read(void) | LogicalChannel_Base |
~LogicalChannel() | NAFE33352_Base::LogicalChannel | virtual
~LogicalChannel_Base() | LogicalChannel_Base | inline virtual