# ShellyBLU H&T

|Model Id|[SBHT-003C](https://github.com/theengs/decoder/blob/development/src/devices/SBHT_003C_json.h)|
|-|-|
|Brand|Shelly|
|Model|ShellyBLU H&T|
|Short Description|Humidity and temperature sensor|
|Communication|BLE broadcast|
|Frequency|2.4Ghz|
|Power Source|CR2032|
|Exchanged Data|temperature, humidity, button press type, battery, packet ID|
|Encrypted|Yes/No - Optional|

The button press type is encoded as:

* 1 - Single short click
* 11 - Button hold
