# RuuviTag (RAWv2 data format)

|Model Id|[RuuviTag_RAWv2](https://github.com/theengs/decoder/blob/development/src/devices/RuuviTag_RAWv2_json.h)|
|-|-|
|Brand|Ruuvi|
|Model|RuuviTag|
|Short Description| Open source environmental sensor|
|Communication|BLE broadcast|
|Frequency|2.4Ghz|
|Power Source|CR2477|
|Exchanged Data|temperature, humidity, pressure, acceleration x/y/z-axis, voltage, TX power, movement counter, measurement sequence number|
|Encrypted|No|
|Device Tracker|&#9989;|
