MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_info_reg Union Reference

INFO (0x0F) page 42. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t c1: 2
uint32_t c2: 4
uint32_t n1: 4
uint32_t n2: 4
uint32_t n3: 4
uint32_t n4: 2
uint32_t reserved: 8
uint32_t revision: 4
} | bit

## Detailed Description

INFO (0x0F) page 42.

## Member Data Documentation

## ◆ all

uint32_t max30001_info_reg::all

## ◆

struct { ... } max30001_info_reg::bit

## ◆ c1

uint32_t max30001_info_reg::c1

## ◆ c2

uint32_t max30001_info_reg::c2

## ◆ n1

uint32_t max30001_info_reg::n1

## ◆ n2

uint32_t max30001_info_reg::n2

## ◆ n3

uint32_t max30001_info_reg::n3

## ◆ n4

uint32_t max30001_info_reg::n4

## ◆ reserved

uint32_t max30001_info_reg::reserved

## ◆ revision

uint32_t max30001_info_reg::revision

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h