MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_gen_reg_t Union Reference

CNFG_GEN (0x10) page 47. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t en_bioz: 1
uint32_t en_bloff: 2
uint32_t en_dcloff: 2
uint32_t en_ecg: 1
uint32_t en_pace: 1
uint32_t en_rbias: 2
uint32_t en_ulp_lon: 2
uint32_t fmstr: 2
uint32_t imag: 3
uint32_t ipol: 1
uint32_t rbiasn: 1
uint32_t rbiasp: 1
uint32_t rbiasv: 2
uint32_t reserved1: 1
uint32_t reserved3: 8
uint32_t vth: 2
} | bit

## Detailed Description

CNFG_GEN (0x10) page 47.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_gen_reg_t::all

## ◆

struct { ... } max30001_cnfg_gen_reg_t::bit

## ◆ en_bioz

uint32_t max30001_cnfg_gen_reg_t::en_bioz

## ◆ en_bloff

uint32_t max30001_cnfg_gen_reg_t::en_bloff

## ◆ en_dcloff

uint32_t max30001_cnfg_gen_reg_t::en_dcloff

## ◆ en_ecg

uint32_t max30001_cnfg_gen_reg_t::en_ecg

## ◆ en_pace

uint32_t max30001_cnfg_gen_reg_t::en_pace

## ◆ en_rbias

uint32_t max30001_cnfg_gen_reg_t::en_rbias

## ◆ en_ulp_lon

uint32_t max30001_cnfg_gen_reg_t::en_ulp_lon

## ◆ fmstr

uint32_t max30001_cnfg_gen_reg_t::fmstr

## ◆ imag

uint32_t max30001_cnfg_gen_reg_t::imag

## ◆ ipol

uint32_t max30001_cnfg_gen_reg_t::ipol

## ◆ rbiasn

uint32_t max30001_cnfg_gen_reg_t::rbiasn

## ◆ rbiasp

uint32_t max30001_cnfg_gen_reg_t::rbiasp

## ◆ rbiasv

uint32_t max30001_cnfg_gen_reg_t::rbiasv

## ◆ reserved1

uint32_t max30001_cnfg_gen_reg_t::reserved1

## ◆ reserved3

uint32_t max30001_cnfg_gen_reg_t::reserved3

## ◆ vth

uint32_t max30001_cnfg_gen_reg_t::vth

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h