MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
ConfigSnapshot Struct Reference

ConfigSnapshot structure for storing/restoring MAX30001G register configurations. More...

`#include <max30001g_typedefs.h>`

## Public Attributes
uint32_t | cnfg_bioz
uint32_t | cnfg_bioz_lc
uint32_t | cnfg_bmux
uint32_t | cnfg_cal
uint32_t | cnfg_ecg
uint32_t | cnfg_emux
uint32_t | cnfg_gen
uint32_t | cnfg_rtor1
uint32_t | cnfg_rtor2
uint32_t | en_int1
uint32_t | en_int2
uint32_t | mngr_dyn
uint32_t | mngr_int
bool | valid

## Detailed Description

ConfigSnapshot structure for storing/restoring MAX30001G register configurations.

Contains key configuration registers that define the device's operating state.

Used for saving/restoring configurations during impedance scans or other operations that modify settings.

## Member Data Documentation

## ◆ cnfg_bioz

uint32_t ConfigSnapshot::cnfg_bioz

## ◆ cnfg_bioz_lc

uint32_t ConfigSnapshot::cnfg_bioz_lc

## ◆ cnfg_bmux

uint32_t ConfigSnapshot::cnfg_bmux

## ◆ cnfg_cal

uint32_t ConfigSnapshot::cnfg_cal

## ◆ cnfg_ecg

uint32_t ConfigSnapshot::cnfg_ecg

## ◆ cnfg_emux

uint32_t ConfigSnapshot::cnfg_emux

## ◆ cnfg_gen

uint32_t ConfigSnapshot::cnfg_gen

## ◆ cnfg_rtor1

uint32_t ConfigSnapshot::cnfg_rtor1

## ◆ cnfg_rtor2

uint32_t ConfigSnapshot::cnfg_rtor2

## ◆ en_int1

uint32_t ConfigSnapshot::en_int1

## ◆ en_int2

uint32_t ConfigSnapshot::en_int2

## ◆ mngr_dyn

uint32_t ConfigSnapshot::mngr_dyn

## ◆ mngr_int

uint32_t ConfigSnapshot::mngr_int

## ◆ valid

bool ConfigSnapshot::valid

The documentation for this struct was generated from the following file:

- src/max30001g_typedefs.h