MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_ecg_burst_reg Union Reference

ECG_FIFO_BURST page 61. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t data: 18
uint32_t etag: 3
uint32_t reserved: 3
} | bit

## Detailed Description

ECG_FIFO_BURST page 61.

## Member Data Documentation

## ◆ all

uint32_t max30001_ecg_burst_reg::all

## ◆

struct { ... } max30001_ecg_burst_reg::bit

## ◆ data

uint32_t max30001_ecg_burst_reg::data

## ◆ etag

uint32_t max30001_ecg_burst_reg::etag

## ◆ reserved

uint32_t max30001_ecg_burst_reg::reserved

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h