MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Here is a list of all class members with links to the classes they belong to:

### - s -

- samp : max30001_status_reg_t
- samp_it : max30001_mngr_int_reg_t
- saveConfig() : MAX30001G
- scanBIOZ() : MAX30001G
- serviceAllInterrupts() : MAX30001G
- servicePendingInterrupts() : MAX30001G
- setBIOZCurrentMonitor() : MAX30001G
- setBIOZfilter() : MAX30001G
- setBIOZgain() : MAX30001G
- setBIOZmag() : MAX30001G
- setBIOZmodulation() : MAX30001G
- setBIOZModulationFrequencyByFrequency() : MAX30001G
- setBIOZModulationFrequencybyIndex() : MAX30001G
- setBIOZPhaseOffsetbyIndex() : MAX30001G
- setBIOZPhaseOffsetbyPhase() : MAX30001G
- setBIOZSamplingRate() : MAX30001G
- setBIOZTestImpedance() : MAX30001G
- setDefaultBIOZTestImpedance() : MAX30001G
- setDefaultBIOZTestSignal() : MAX30001G
- setDefaultECGandBIOZTestSignal() : MAX30001G
- setDefaultECGTestSignal() : MAX30001G
- setDefaultInterruptClearing() : MAX30001G
- setDefaultNoBIOZTestImpedance() : MAX30001G
- setDefaultNoRtoR() : MAX30001G
- setDefaultNoTestSignal() : MAX30001G
- setDefaultRtoR() : MAX30001G
- setECGAutoRecovery() : MAX30001G
- setECGfilter() : MAX30001G
- setECGgain() : MAX30001G
- setECGLeadPolarity() : MAX30001G
- setECGNormalRecovery() : MAX30001G
- setECGSamplingRate() : MAX30001G
- setFIFOInterruptThreshold() : MAX30001G
- setFMSTR() : MAX30001G
- setInterrupt1() : MAX30001G
- setInterrupt2() : MAX30001G
- setInterruptAggregateCallback() : MAX30001G
- setInterruptEventCallback() : MAX30001G
- setLeadsBias() : MAX30001G
- setLeadsOffDetection() : MAX30001G
- setLeadsOnDetection() : MAX30001G
- setRtoR() : MAX30001G
- setTestSignal() : MAX30001G
- setupBIOZ() : MAX30001G
- setupBIOZExternalImpedanceCalibration() : MAX30001G
- setupBIOZImpedanceCalibration() : MAX30001G
- setupBIOZScan() : MAX30001G
- setupBIOZSignalCalibration() : MAX30001G
- setupECG() : MAX30001G
- setupECGandBIOZ() : MAX30001G
- setupECGSignalCalibration() : MAX30001G
- spi_ok : HealthCheckResult
- start() : MAX30001G
- startBIOZScan() : MAX30001G
- startECGManualRecovery() : MAX30001G
- status_reg : HealthCheckResult
- stepBIOZScan() : MAX30001G
- stop() : MAX30001G
- stopBIOZScan() : MAX30001G
- stopECGManualRecovery() : MAX30001G
- swReset() : MAX30001G
- synch() : MAX30001G