MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Here is a list of all class members with links to the classes they belong to:

### - c -

- c1 : max30001_info_reg
- c2 : max30001_info_reg
- caln_sel : max30001_cnfg_bmux_reg_t , max30001_cnfg_emux_reg
- calp_sel : max30001_cnfg_bmux_reg_t , max30001_cnfg_emux_reg
- capacity() : RingBuffer< T, N >
- cg_mode : max30001_cnfg_bmux_reg_t
- cgmag : max30001_cnfg_bioz_reg_t
- cgmon : max30001_cnfg_bioz_reg_t
- clear() : RingBuffer< T, N >
- clearAllInterruptCallbacks() : MAX30001G
- clearInterruptAggregateCallback() : MAX30001G
- clearInterruptEventCallback() : MAX30001G
- clearLatchedStatusFlags() : MAX30001G
- clr_fast : max30001_mngr_int_reg_t
- clr_pedge : max30001_mngr_int_reg_t
- clr_rrint : max30001_mngr_int_reg_t
- clr_samp : max30001_mngr_int_reg_t
- cmag_lc : max30001_cnfg_bioz_lc_reg_t
- cmres : max30001_cnfg_bioz_lc_reg_t
- cnfg_bioz : ConfigSnapshot
- cnfg_bioz_lc : ConfigSnapshot
- cnfg_bmux : ConfigSnapshot
- cnfg_cal : ConfigSnapshot
- cnfg_ecg : ConfigSnapshot
- cnfg_emux : ConfigSnapshot
- cnfg_gen : ConfigSnapshot
- cnfg_rtor1 : ConfigSnapshot
- cnfg_rtor2 : ConfigSnapshot
- consume() : RingBuffer< T, N >