MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_mngr_dyn_reg_t Union Reference

MNGR_DYN (0x05) page 45. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t bloff_hi_it: 8
uint32_t bloff_lo_it: 8
uint32_t fast: 2
uint32_t fast_th: 6
uint32_t reserved: 8
} | bit

## Detailed Description

MNGR_DYN (0x05) page 45.

## Member Data Documentation

## ◆ all

uint32_t max30001_mngr_dyn_reg_t::all

## ◆

struct { ... } max30001_mngr_dyn_reg_t::bit

## ◆ bloff_hi_it

uint32_t max30001_mngr_dyn_reg_t::bloff_hi_it

## ◆ bloff_lo_it

uint32_t max30001_mngr_dyn_reg_t::bloff_lo_it

## ◆ fast

uint32_t max30001_mngr_dyn_reg_t::fast

## ◆ fast_th

uint32_t max30001_mngr_dyn_reg_t::fast_th

## ◆ reserved

uint32_t max30001_mngr_dyn_reg_t::reserved

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h