MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
ImpedanceSpectrum Struct Reference

ImpedanceSpectrum structure for storing one full BIOZ sweep. More...

`#include <max30001g_typedefs.h>`

## Public Attributes
float | frequency [MAX30001_BIOZ_NUM_FREQUENCIES]
float | magnitude [MAX30001_BIOZ_NUM_FREQUENCIES]
float | phase [MAX30001_BIOZ_NUM_FREQUENCIES]

## Detailed Description

ImpedanceSpectrum structure for storing one full BIOZ sweep.

Each index corresponds to one modulation frequency bin with fitted magnitude and phase.

## Member Data Documentation

## ◆ frequency

float ImpedanceSpectrum::frequency[MAX30001_BIOZ_NUM_FREQUENCIES]

## ◆ magnitude

float ImpedanceSpectrum::magnitude[MAX30001_BIOZ_NUM_FREQUENCIES]

## ◆ phase

float ImpedanceSpectrum::phase[MAX30001_BIOZ_NUM_FREQUENCIES]

The documentation for this struct was generated from the following file:

- src/max30001g_typedefs.h