MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Here is a list of all class members with links to the classes they belong to:

### - i -

- imag : max30001_cnfg_gen_reg_t
- info_reg : HealthCheckResult
- initial_current_nA : BIOZScanConfig
- intb_type : max30001_en_int_reg_t
- internal_resistor_ohm : BIOZScanConfig
- InterruptCallback : MAX30001G
- InterruptEvent : MAX30001G
- ipol : max30001_cnfg_gen_reg_t
- IRQ_BIOZ_CGMON : MAX30001G
- IRQ_BIOZ_FIFO : MAX30001G
- IRQ_BIOZ_OVER : MAX30001G
- IRQ_BIOZ_OVF : MAX30001G
- IRQ_BIOZ_UNDER : MAX30001G
- IRQ_ECG_FAST : MAX30001G
- IRQ_ECG_FIFO : MAX30001G
- IRQ_ECG_LEADOFF : MAX30001G
- IRQ_ECG_OVF : MAX30001G
- IRQ_EVENT_COUNT : MAX30001G
- IRQ_LEADS_ON : MAX30001G
- IRQ_PLL_UNLOCK : MAX30001G
- IRQ_RTOR : MAX30001G