MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_cal_reg_t Union Reference

CNFG_CAL (0x12) page 49. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t fcal: 3
uint32_t fifty: 1
uint32_t reserved1: 5
uint32_t reserved2: 1
uint32_t reserved3: 8
uint32_t thigh: 11
uint32_t vcal: 1
uint32_t vmag: 1
uint32_t vmode: 1
} | bit

## Detailed Description

CNFG_CAL (0x12) page 49.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_cal_reg_t::all

## ◆

struct { ... } max30001_cnfg_cal_reg_t::bit

## ◆ fcal

uint32_t max30001_cnfg_cal_reg_t::fcal

## ◆ fifty

uint32_t max30001_cnfg_cal_reg_t::fifty

## ◆ reserved1

uint32_t max30001_cnfg_cal_reg_t::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_cal_reg_t::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_cal_reg_t::reserved3

## ◆ thigh

uint32_t max30001_cnfg_cal_reg_t::thigh

## ◆ vcal

uint32_t max30001_cnfg_cal_reg_t::vcal

## ◆ vmag

uint32_t max30001_cnfg_cal_reg_t::vmag

## ◆ vmode

uint32_t max30001_cnfg_cal_reg_t::vmode

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h