MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_emux_reg Union Reference

CNFG_EMUX (0x14) page 50. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t caln_sel: 2
uint32_t calp_sel: 2
uint32_t openn: 1
uint32_t openp: 1
uint32_t pol: 1
uint32_t reserved1: 16
uint32_t reserved2: 1
uint32_t reserved3: 8
} | bit

## Detailed Description

CNFG_EMUX (0x14) page 50.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_emux_reg::all

## ◆

struct { ... } max30001_cnfg_emux_reg::bit

## ◆ caln_sel

uint32_t max30001_cnfg_emux_reg::caln_sel

## ◆ calp_sel

uint32_t max30001_cnfg_emux_reg::calp_sel

## ◆ openn

uint32_t max30001_cnfg_emux_reg::openn

## ◆ openp

uint32_t max30001_cnfg_emux_reg::openp

## ◆ pol

uint32_t max30001_cnfg_emux_reg::pol

## ◆ reserved1

uint32_t max30001_cnfg_emux_reg::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_emux_reg::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_emux_reg::reserved3

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h