MAX30001G 1.0.2 Arduino library for MAX30001G ECG and BIOZ AFE

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:

C BIOZScanConfig | BIOZScanConfig configuration structure fields:
C ConfigSnapshot | ConfigSnapshot structure for storing/restoring MAX30001G register configurations
C HealthCheckResult | HealthCheckResult structure for storing health check results
C ImpedanceModel | ImpedanceModel structure for storing impedance measurement results
C ImpedanceSpectrum | ImpedanceSpectrum structure for storing one full BIOZ sweep
C max30001_bioz_burst_reg_t | BIOZ_FIFO_BURST page 61
C max30001_cnfg_bioz_lc_reg_t | CNFG_BIOZ_LC (0x1A) page 57
C max30001_cnfg_bioz_reg_t | CNFG_BIOZ (0x18) page 54
C max30001_cnfg_bmux_reg_t | CNFG_BMUX (0x17) page 52
C max30001_cnfg_cal_reg_t | CNFG_CAL (0x12) page 49
C max30001_cnfg_ecg_reg | CNFG_ECG (0x15) page 51
C max30001_cnfg_emux_reg | CNFG_EMUX (0x14) page 50
C max30001_cnfg_gen_reg_t | CNFG_GEN (0x10) page 47
C max30001_cnfg_rtor1_reg_t | CNFG_RTOR1 (0x1D) page 59
C max30001_cnfg_rtor2_reg_t | CNFG_RTOR2 (0x1E) page 59
C max30001_ecg_burst_reg | ECG_FIFO_BURST page 61
C max30001_en_int_reg_t | EN_INT (0x02) and (0x03) page 43 we can attach two interrupt lines to functions of the MAX30001 multiple interrupts can be enabled at the same time as the bits are OR-ed
C max30001_info_reg | INFO (0x0F) page 42
C max30001_mngr_dyn_reg_t | MNGR_DYN (0x05) page 45
C max30001_mngr_int_reg_t | MNGR_INT (0x04) page 44
C max30001_rtor_reg | R to R FIFO page 61
C max30001_status_reg_t | STATUS (0x01) page 42
C MAX30001G | MAX30001G device driver class used by Arduino sketches
C RingBuffer |