MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Classes | Enumerations
max30001g_typedefs.h File Reference
`#include <stdint.h>`
`#include "max30001g_defs.h"`
Include dependency graph for max30001g_typedefs.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Classes
struct | BIOZScanConfig
| BIOZScanConfig configuration structure fields: More...
struct | ConfigSnapshot
| ConfigSnapshot structure for storing/restoring MAX30001G register configurations. More...
struct | HealthCheckResult
| HealthCheckResult structure for storing health check results. More...
struct | ImpedanceModel
| ImpedanceModel structure for storing impedance measurement results. More...
struct | ImpedanceSpectrum
| ImpedanceSpectrum structure for storing one full BIOZ sweep. More...

## Enumerations
enum | BIOZScanPhaseRange : uint8_t { BIOZ_SCAN_PHASE_FULL = 0 , BIOZ_SCAN_PHASE_REDUCED }
| BIOZ scan phase-density selection. More...

## Enumeration Type Documentation

## ◆ BIOZScanPhaseRange

enum BIOZScanPhaseRange : uint8_t

BIOZ scan phase-density selection.

FULL uses all hardware-supported phase offsets for the active FCGEN.

REDUCED uses four 45 degree steps: 0, 45, 90, and 135 degrees.

Enumerator
BIOZ_SCAN_PHASE_FULL |
BIOZ_SCAN_PHASE_REDUCED |