MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_bmux_reg_t Union Reference

CNFG_BMUX (0x17) page 52. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t caln_sel: 2
uint32_t calp_sel: 2
uint32_t cg_mode: 2
uint32_t en_bist: 1
uint32_t fbist: 2
uint32_t openn: 1
uint32_t openp: 1
uint32_t reserved: 8
uint32_t reserved1: 2
uint32_t reserved2: 1
uint32_t reserved3: 2
uint32_t reserved4: 2
uint32_t rmod: 3
uint32_t rnom: 3
} | bit

## Detailed Description

CNFG_BMUX (0x17) page 52.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_bmux_reg_t::all

## ◆

struct { ... } max30001_cnfg_bmux_reg_t::bit

## ◆ caln_sel

uint32_t max30001_cnfg_bmux_reg_t::caln_sel

## ◆ calp_sel

uint32_t max30001_cnfg_bmux_reg_t::calp_sel

## ◆ cg_mode

uint32_t max30001_cnfg_bmux_reg_t::cg_mode

## ◆ en_bist

uint32_t max30001_cnfg_bmux_reg_t::en_bist

## ◆ fbist

uint32_t max30001_cnfg_bmux_reg_t::fbist

## ◆ openn

uint32_t max30001_cnfg_bmux_reg_t::openn

## ◆ openp

uint32_t max30001_cnfg_bmux_reg_t::openp

## ◆ reserved

uint32_t max30001_cnfg_bmux_reg_t::reserved

## ◆ reserved1

uint32_t max30001_cnfg_bmux_reg_t::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_bmux_reg_t::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_bmux_reg_t::reserved3

## ◆ reserved4

uint32_t max30001_cnfg_bmux_reg_t::reserved4

## ◆ rmod

uint32_t max30001_cnfg_bmux_reg_t::rmod

## ◆ rnom

uint32_t max30001_cnfg_bmux_reg_t::rnom

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h