MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Here is a list of all class members with links to the classes they belong to:

### - p -

- pavg : max30001_cnfg_rtor1_reg_t
- pedge : max30001_status_reg_t
- phase : ImpedanceModel , ImpedanceSpectrum
- phase_range : BIOZScanConfig
- phoff : max30001_cnfg_bioz_reg_t
- pll_unlocked : HealthCheckResult
- pllint : max30001_status_reg_t
- pol : max30001_cnfg_emux_reg
- povf : max30001_status_reg_t
- print : max30001_status_reg_t
- printAllRegisters() : MAX30001G
- printBiozDiagnosticRegisters() : MAX30001G
- printConfig() : MAX30001G
- printInfo() : MAX30001G
- printStatus() : MAX30001G
- ptsf : max30001_cnfg_rtor1_reg_t