MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Public Types | Public Member Functions | List of all members
MAX30001G Class Reference
MAX30001G Public API

MAX30001G device driver class used by Arduino sketches. More...

`#include <max30001g.h>`

## Public Types
typedef void(* | InterruptCallback) (MAX30001G *device, uint32_t status, void *context)
enum | InterruptEvent : uint8_t { IRQ_ECG_FIFO = 0 , IRQ_ECG_OVF , IRQ_ECG_FAST , IRQ_ECG_LEADOFF , IRQ_BIOZ_FIFO , IRQ_BIOZ_OVF , IRQ_BIOZ_OVER , IRQ_BIOZ_UNDER , IRQ_BIOZ_CGMON , IRQ_LEADS_ON , IRQ_RTOR , IRQ_PLL_UNLOCK , IRQ_EVENT_COUNT }

## Public Member Functions
void | begin (void)
void | clearAllInterruptCallbacks (void)
| Clear all registered interrupt callbacks for this instance. More...
void | clearInterruptAggregateCallback (void)
| Clear aggregate interrupt callback. More...
void | clearInterruptEventCallback (InterruptEvent event)
| Clear callback for one interrupt event. More...
void | clearLatchedStatusFlags (void)
| Clear software-latched interrupt/fault flags. More...
void | enableAFE (bool ECG, bool BIOZ, bool RtoR)
| Enable or disable ECG, BIOZ, and R-to-R engines. More...
void | end (void)
void | FIFOReset (void)
| Reset ECG and BIOZ FIFOs. Does not affect data already transferred to RingBuffer. More...
void | handleBIOZFifoInterrupt (bool reportRaw=false)
| Convenience callback handler: read BIOZ FIFO. More...
void | handleECGFifoInterrupt (bool reportRaw=false)
| Convenience callback handler: read ECG FIFO. More...
void | handleRtoRInterrupt (void)
| Convenience callback handler: read RTOR data. More...
HealthCheckResult | healthCheck (void)
| Run basic health checks and return a summary result. More...
| MAX30001G (uint8_t csPin, int intPin1=-1, int intPin2=-1)
| Construct a MAX30001G device instance. More...
void | printAllRegisters (void)
void | printBiozDiagnosticRegisters (const char *context=nullptr)
void | printConfig (void)
void | printInfo (void)
void | printStatus (void)
void | readAllRegisters (void)
void | readAndClearFaults (void)
| Read and clear fault-related status conditions. More...
float | readBIOZ (bool reportRaw)
| Read one BIOZ FIFO sample. More...
void | readBIOZ_FIFO (bool reportRaw)
| Burst-read BIOZ FIFO samples. More...
float | readECG (bool reportRaw)
| Read one ECG FIFO sample. More...
void | readECG_FIFO (bool reportRaw)
| Burst-read ECG FIFO samples. More...
void | readInfo (void)
void | readRTOR (void)
| Read RTOR result and update RR-interval globals/buffer. More...
void | readStatusRegisters (void)
void | restoreConfig (void)
void | saveConfig (void)
void | serviceAllInterrupts (void)
| Read STATUS and update interrupt-driven global flags. More...
bool | servicePendingInterrupts (void)
| Service interrupts only when ISR software flags indicate pending work. More...
void | setBIOZCurrentMonitor (bool enable)
| Enable/disable BIOZ current monitor. More...
void | setBIOZfilter (uint8_t ahpf, uint8_t lpf, uint8_t hpf)
| Configure BIOZ analog and digital filters. More...
void | setBIOZgain (uint8_t gain, bool lowNoise)
| Set BIOZ gain and front-end power/noise mode. More...
void | setBIOZmag (uint32_t current_nA)
| Set BIOZ current magnitude. More...
void | setBIOZmodulation (uint8_t mode)
| Set BIOZ current-generator modulation mode. More...
void | setBIOZModulationFrequencyByFrequency (uint32_t frequency_hz)
| Set BIOZ modulation frequency by target Hz. More...
void | setBIOZModulationFrequencybyIndex (uint8_t frequency_selector)
| Set BIOZ modulation frequency by FCGEN index. More...
void | setBIOZPhaseOffsetbyIndex (uint8_t selector)
| Set BIOZ demodulation phase by selector. More...
void | setBIOZPhaseOffsetbyPhase (float phase_deg)
| Set BIOZ demodulation phase by degree request. More...
void | setBIOZPhaseOffsetbyPhase (uint32_t frequency_hz, float phase_deg)
| Set BIOZ demodulation phase by explicit frequency and phase. More...
void | setBIOZSamplingRate (uint8_t speed_select)
| Set BIOZ sample-rate selector. More...
void | setBIOZTestImpedance (bool enable, bool useHighResistance, bool enableModulation, uint8_t rnomValue, uint8_t rmodValue, uint8_t modFreq)
| Configure BIOZ test impedance and optional modulation. More...
void | setDefaultBIOZTestImpedance (void)
| Apply default internal BIOZ test impedance settings. More...
void | setDefaultBIOZTestSignal (void)
| Apply default BIOZ voltage calibration signal settings. More...
void | setDefaultECGandBIOZTestSignal (void)
| Apply default voltage calibration settings to ECG and BIOZ. More...
void | setDefaultECGTestSignal (void)
| Apply default ECG voltage calibration signal settings. More...
void | setDefaultInterruptClearing (void)
| Configure default interrupt-clear, clears on RR read, fast recovery read, and sample read. More...
void | setDefaultNoBIOZTestImpedance (void)
| Disable internal BIOZ test impedance path. More...
void | setDefaultNoRtoR (void)
| Apply default RTOR settings with RTOR disabled. More...
void | setDefaultNoTestSignal (void)
| Disable ECG/BIOZ voltage calibration source routing. More...
void | setDefaultRtoR (void)
| Apply default RTOR settings and enable RTOR detection. More...
void | setECGAutoRecovery (int threshold_voltage)
| Enable automatic ECG fast-recovery mode. More...
void | setECGfilter (uint8_t lpf, uint8_t hpf)
| Configure ECG digital filters. More...
void | setECGgain (uint8_t gain)
| Set ECG PGA gain. More...
void | setECGLeadPolarity (bool inverted, bool open)
| Configure ECG polarity and input switch state. More...
void | setECGNormalRecovery (void)
void | setECGSamplingRate (uint8_t ECG)
| Set ECG sample-rate selector. More...
void | setFIFOInterruptThreshold (uint8_t ecg, uint8_t bioz)
| Set FIFO threshold that triggers ECG/BIOZ FIFO interrupts. More...
void | setFMSTR (uint8_t fmstr)
| Set master clock selector and recompute timing globals. More...
bool | setInterrupt1 (bool ecg, bool bioz, bool rtor, bool leadon, bool leadoff, bool bioz_fourwire=false)
| Configure interrupt line INT1 event enables. More...
bool | setInterrupt2 (bool ecg, bool bioz, bool rtor, bool leadon, bool leadoff, bool bioz_fourwire=false)
| Configure interrupt line INT2 event enables. More...
bool | setInterruptAggregateCallback (InterruptCallback cb, void *context=nullptr, uint32_t statusMask=0x00FFFFFFUL)
| Register aggregate callback invoked for status bits matching a mask. More...
bool | setInterruptEventCallback (InterruptEvent event, InterruptCallback cb, void *context=nullptr)
| Register callback for one specific interrupt event. More...
void | setLeadsBias (bool enable, uint8_t resistance)
| Configure lead-bias mode and resistance. More...
void | setLeadsOffDetection (bool enable, bool bioz_4, uint8_t electrode_impedance)
| Configure lead-off detection behavior. More...
void | setLeadsOnDetection (bool enable)
| Enable/disable ultra-low-power lead-on detection. More...
void | setRtoR (bool enable, uint8_t ptsf, uint8_t pavg, uint8_t gain, uint8_t wndw, uint8_t hoff, uint8_t ravg, uint8_t rhsf)
| Configure RTOR algorithm parameters. More...
void | setTestSignal (bool enableECGCalSignal, bool enableBIOZCalSignal, bool unipolar, bool cal_vmag, uint8_t freq, uint8_t dutycycle)
| Configure calibration voltage source and waveform settings. More...
void | setupBIOZ (uint8_t speed=0, uint8_t gain=1, uint8_t ahpf=1, uint8_t dlpf=1, uint8_t dhpf=0, uint32_t frequency=40000, uint32_t current=8000, float phase=0.0f, bool leadbias=true, bool leadsoffdetect=false, bool fourleads=false)
| Configure a ready-to-use BIOZ profile. More...
void | setupBIOZExternalImpedanceCalibration (uint32_t frequency=40000, float phase=0.0f)
| Configure external impedance calibration path. More...
void | setupBIOZImpedanceCalibration (uint8_t speed=0, uint8_t gain=1, uint8_t ahpf=1, uint8_t dlpf=1, uint8_t dhpf=0, uint32_t frequency=40000, uint32_t current=8000, float phase=0.0f, uint32_t resistance=5000, uint8_t modulation=0, uint8_t modulation_frequency=3)
| Configure internal BIOZ impedance calibration/test path. More...
void | setupBIOZScan (const BIOZScanConfig &config=BIOZScanConfig(), bool reuseCurrents=false)
| Configure lifecycle-driven BIOZ scan flow. More...
void | setupBIOZScan (uint8_t avg, bool fast, bool fourleads, bool fullRange)
| Configure lifecycle-driven BIOZ scan flow. More...
void | setupBIOZSignalCalibration (uint8_t speed=0, uint8_t gain=1)
| Configure BIOZ voltage calibration signal path. More...
void | setupECG (uint8_t speed=1, uint8_t gain=2, bool threeleads=true)
| Configure a ready-to-use ECG profile. More...
void | setupECGandBIOZ (uint8_t ecg_speed=1, uint8_t ecg_gain=2, bool ecg_threeleads=true, uint8_t bioz_speed=0, uint8_t bioz_gain=1, uint8_t bioz_dlpf=1, uint8_t bioz_dhpf=0, uint32_t bioz_frequency=8000, uint32_t bioz_current=8000, float bioz_phase=0.0f, bool leadbias=true, bool leadsoffdetect=false, bool bioz_fourleads=false)
| Configure simultaneous ECG and BIOZ operation. More...
void | setupECGSignalCalibration (uint8_t speed=1, uint8_t gain=2)
| Configure ECG voltage calibration signal path. More...
void | start (void)
| Start measurement engines according to the most recent setup profile. More...
void | startBIOZScan (void)
| Start state-machine style BIOZ scan flow. More...
void | startECGManualRecovery (void)
void | stepBIOZScan (void)
| Advance state-machine style BIOZ scan flow by one step. More...
void | stop (void)
| Stop active measurement engines. More...
void | stopBIOZScan (void)
| Stop state-machine style BIOZ scan flow. More...
void | stopECGManualRecovery (void)
void | swReset (void)
void | synch (void)
bool | update (bool reportRaw=false)
| Service pending IRQ work and drain enabled FIFOs. More...
bool | updateRaw (void)
| Alias for raw-code update cycle. More...

## Detailed Description

MAX30001G device driver class used by Arduino sketches.

## Member Typedef Documentation

## ◆ InterruptCallback

typedef void(* MAX30001G::InterruptCallback) (MAX30001G *device, uint32_t status, void *context)

## Member Enumeration Documentation

## ◆ InterruptEvent

enum MAX30001G::InterruptEvent : uint8_t

Enumerator
IRQ_ECG_FIFO |
IRQ_ECG_OVF |
IRQ_ECG_FAST |
IRQ_ECG_LEADOFF |
IRQ_BIOZ_FIFO |
IRQ_BIOZ_OVF |
IRQ_BIOZ_OVER |
IRQ_BIOZ_UNDER |
IRQ_BIOZ_CGMON |
IRQ_LEADS_ON |
IRQ_RTOR |
IRQ_PLL_UNLOCK |
IRQ_EVENT_COUNT |

## Constructor & Destructor Documentation

## ◆ MAX30001G()

MAX30001G::MAX30001G | ( | uint8_t | csPin,
|  | int | intPin1 = `-1`,
|  | int | intPin2 = `-1`
| ) |  |

Construct a MAX30001G device instance.

Parameters

  csPin | SPI chip-select pin.
  intPin1 | Optional INTB pin number. Use -1 when not connected.
  intPin2 | Optional INT2B pin number. Use -1 when not connected.

## Member Function Documentation

## ◆ begin()

void MAX30001G::begin | ( | void |  | ) |

## ◆ clearAllInterruptCallbacks()

void MAX30001G::clearAllInterruptCallbacks | ( | void |  | ) |

Clear all registered interrupt callbacks for this instance.

## ◆ clearInterruptAggregateCallback()

void MAX30001G::clearInterruptAggregateCallback | ( | void |  | ) |

Clear aggregate interrupt callback.

## ◆ clearInterruptEventCallback()

void MAX30001G::clearInterruptEventCallback | ( | InterruptEvent | event | ) |

Clear callback for one interrupt event.

event must be one value from InterruptEvent.

Parameters

  event | Interrupt event selector.

## ◆ clearLatchedStatusFlags()

void MAX30001G::clearLatchedStatusFlags | ( | void |  | ) |

Clear software-latched interrupt/fault flags.

This does not read/write device registers; it only resets library globals that are latched by STATUS/FIFO parsing.

## ◆ enableAFE()

void MAX30001G::enableAFE | ( | bool | ECG,
|  | bool | BIOZ,
|  | bool | RtoR
| ) |  |

Enable or disable ECG, BIOZ, and R-to-R engines.

Parameters

  ECG | True to enable ECG path.
  BIOZ | True to enable BIOZ path.
  RtoR | True to enable R-to-R detection.

## ◆ end()

void MAX30001G::end | ( | void |  | ) |

## ◆ FIFOReset()

void MAX30001G::FIFOReset | ( | void |  | ) |

Reset ECG and BIOZ FIFOs. Does not affect data already transferred to RingBuffer.

## ◆ handleBIOZFifoInterrupt()

void MAX30001G::handleBIOZFifoInterrupt | ( | bool | reportRaw = `false` | ) |

Convenience callback handler: read BIOZ FIFO.

Parameters

  reportRaw | True to keep ADC codes; false to convert.

## ◆ handleECGFifoInterrupt()

void MAX30001G::handleECGFifoInterrupt | ( | bool | reportRaw = `false` | ) |

Convenience callback handler: read ECG FIFO.

Parameters

  reportRaw | True to keep ADC codes; false to convert.

## ◆ handleRtoRInterrupt()

void MAX30001G::handleRtoRInterrupt | ( | void |  | ) |

Convenience callback handler: read RTOR data.

## ◆ healthCheck()

HealthCheckResult MAX30001G::healthCheck | ( | void |  | ) |

Run basic health checks and return a summary result.

Returns
  HealthCheckResult with SPI, INFO, STATUS, and fault summary fields.

## ◆ printAllRegisters()

void MAX30001G::printAllRegisters | ( | void |  | ) |

## ◆ printBiozDiagnosticRegisters()

void MAX30001G::printBiozDiagnosticRegisters | ( | const char * | context = `nullptr` | ) |

## ◆ printConfig()

void MAX30001G::printConfig | ( | void |  | ) |

## ◆ printInfo()

void MAX30001G::printInfo | ( | void |  | ) |

## ◆ printStatus()

void MAX30001G::printStatus | ( | void |  | ) |

## ◆ readAllRegisters()

void MAX30001G::readAllRegisters | ( | void |  | ) |

## ◆ readAndClearFaults()

void MAX30001G::readAndClearFaults | ( | void |  | ) |

Read and clear fault-related status conditions.

## ◆ readBIOZ()

float MAX30001G::readBIOZ | ( | bool | reportRaw | ) |

Read one BIOZ FIFO sample.

Parameters

  reportRaw | True to keep ADC code; false to convert to ohms.

Returns
  Sample value or sentinel for invalid/empty cases.

## ◆ readBIOZ_FIFO()

void MAX30001G::readBIOZ_FIFO | ( | bool | reportRaw | ) |

Burst-read BIOZ FIFO samples.

Parameters

  reportRaw | True to keep ADC codes; false to convert to engineering units.

## ◆ readECG()

float MAX30001G::readECG | ( | bool | reportRaw | ) |

Read one ECG FIFO sample.

Parameters

  reportRaw | True to keep ADC code; false to convert to mV.

Returns
  Sample value or sentinel for invalid/empty cases.

## ◆ readECG_FIFO()

void MAX30001G::readECG_FIFO | ( | bool | reportRaw | ) |

Burst-read ECG FIFO samples.

Parameters

  reportRaw | True to keep ADC codes; false to convert to engineering units.

## ◆ readInfo()

void MAX30001G::readInfo | ( | void |  | ) |

## ◆ readRTOR()

void MAX30001G::readRTOR | ( | void |  | ) |

Read RTOR result and update RR-interval globals/buffer.

## ◆ readStatusRegisters()

void MAX30001G::readStatusRegisters | ( | void |  | ) |

## ◆ restoreConfig()

void MAX30001G::restoreConfig | ( | void |  | ) |

## ◆ saveConfig()

void MAX30001G::saveConfig | ( | void |  | ) |

## ◆ serviceAllInterrupts()

void MAX30001G::serviceAllInterrupts | ( | void |  | ) |

Read STATUS and update interrupt-driven global flags.

## ◆ servicePendingInterrupts()

bool MAX30001G::servicePendingInterrupts | ( | void |  | ) |

Service interrupts only when ISR software flags indicate pending work.

Uses Arduino-core critical-section calls (`noInterrupts()` / `interrupts()`) to atomically snapshot and clear software pending flags.

Returns
  True if an interrupt service pass was performed.

## ◆ setBIOZCurrentMonitor()

void MAX30001G::setBIOZCurrentMonitor | ( | bool | enable | ) |

Enable/disable BIOZ current monitor.

Parameters

  enable | True to enable current monitor path.

## ◆ setBIOZfilter()

void MAX30001G::setBIOZfilter | ( | uint8_t | ahpf,
|  | uint8_t | lpf,
|  | uint8_t | hpf
| ) |  |

Configure BIOZ analog and digital filters.

ahpf (should be lower than selected modulation frequency)

0 60 Hz

1 150 Hz

2 500 Hz

3 1000 Hz

4 2000 Hz

5 4000 Hz

>=6 bypass

dlpf (set higher for fast changing signals, but more noise)

0 bypass

1 4 Hz **

2 8 Hz

3 16 Hz

dhpf (bypass or filter out static content to visualize cardiac induced changes)

0 bypass **

1 0.05Hz

2 0.5Hz

Parameters

  ahpf | Analog HPF selector (0..7). 0:60Hz 1:150Hz 2:500Hz* 3:1000Hz 4:2000Hz 5:4000Hz 6/7:bypass
  lpf | Digital LPF selector (0..3). 0:bypass 1:~4Hz* 2:~8Hz 3:~16Hz
  hpf | Digital HPF selector (0..3). 0:bypass* 1:0.05Hz 2/3:0.5Hz

## ◆ setBIOZgain()

void MAX30001G::setBIOZgain | ( | uint8_t | gain,
|  | bool | lowNoise
| ) |  |

Set BIOZ gain and front-end power/noise mode.

0 10 V/V

1 20 V/V **

2 40 V/V

3 80 V/V

Parameters

  gain | Gain selector (0..3 => 10, 20**, 40, 80 V/V).
  lowNoise | True for low-noise mode, false for low-power mode.

## ◆ setBIOZmag()

void MAX30001G::setBIOZmag | ( | uint32_t | current_nA | ) |

Set BIOZ current magnitude.

current in nanoAmps (8uA works with all settings, higher current is better for measuring low impedance)

55..96,000 nano Amps

8,000 **

Parameters

  current_nA | Requested current in nA (mapped/clamped to valid table values). High-current (8uA..96uA) Low-current range (55nA..1100nA)

## ◆ setBIOZmodulation()

void MAX30001G::setBIOZmodulation | ( | uint8_t | mode | ) |

Set BIOZ current-generator modulation mode.

0 = Unchopped with LPF * (higher noise, excellent 50/60 rejection, recommended for ECG, BIOZ applications)

1 = Chopped without LPF (low noise, poor 50/60Hz rejection, recommended for BIOZ applications, possibly battery powered ECG))

2 = Chopped with LPF (low noise, excellent 50/60Hz rejection)

3 = Chopped with resistive CM (Not recommended to be used for drive currents >32µA, low noise, excellent 50/60Hz rejection, lower input impedance)

Datasheet note: use mode 0 when BIOZ_HI_LOB=0 (low-current range).

Parameters

  mode | BMUX_CG_MODE selector (0..3).

## ◆ setBIOZModulationFrequencyByFrequency()

void MAX30001G::setBIOZModulationFrequencyByFrequency | ( | uint32_t | frequency_hz | ) |

Set BIOZ modulation frequency by target Hz.

frequency (historically data was recorded at 50KHz, any frequency from 125Hz to 128kHz is available)

128,000

80,000

40,000 **

18,000

8,000

4,000

2,000

1,000

500 might have 60/50Hz interference

250 might have 60/50Hz interference

125 might have 60/50Hz interference

Parameters

  frequency_hz | Requested frequency in Hz (mapped to nearest valid FCGEN).

## ◆ setBIOZModulationFrequencybyIndex()

void MAX30001G::setBIOZModulationFrequencybyIndex | ( | uint8_t | frequency_selector | ) |

Set BIOZ modulation frequency by FCGEN index.

selector to frequency mapping:

0=128000Hz, 1=80000Hz, 2=40000Hz, 3=18000Hz, 4=8000Hz,

5=4000Hz, 6=2000Hz, 7=1000Hz, 8=500Hz, 9=250Hz, 10=125Hz.

Parameters

  frequency_selector | FCGEN selector (0..10 valid).

## ◆ setBIOZPhaseOffsetbyIndex()

void MAX30001G::setBIOZPhaseOffsetbyIndex | ( | uint8_t | selector | ) |

Set BIOZ demodulation phase by selector.

FCGEN=0000: selector 0..3 (45.00deg steps) (128kHz)

FCGEN=0001: selector 0..7 (22.50deg steps) (80kHz)

FCGEN>=0010: selector 0..15 (11.25deg steps) (40kHz and lower)

Parameters

  selector | Phase index (range depends on FCGEN).

## ◆ setBIOZPhaseOffsetbyPhase() [1/2]

void MAX30001G::setBIOZPhaseOffsetbyPhase | ( | float | phase_deg | ) |

Set BIOZ demodulation phase by degree request.

phase delay between current and voltage measurement

for accurate phase and impedance reading at least two phase settings

need to be measured, default is no phase shift, just measure real component

phase in degrees

<80kHz 80kHz 128kHz

0 0.00 0.0 0.0 **

1 11.25 22.5 45.0

2 22.50 45.0 90.0

3 33.75 67.5 135.0

4 45.00 90.0

5 56.25 112.5

6 67.50 135.0

7 78.75 157.5

8 90.00

9 101.25

10 112.50

11 123.75

12 135.00

13 146.25

14 157.50

15 168.75

Parameters

  phase_deg | Requested phase in degrees.

## ◆ setBIOZPhaseOffsetbyPhase() [2/2]

void MAX30001G::setBIOZPhaseOffsetbyPhase | ( | uint32_t | frequency_hz,
|  | float | phase_deg
| ) |  |

Set BIOZ demodulation phase by explicit frequency and phase.

Phase-index resolution depends on frequency band:

128kHz uses 4 phases (45deg steps), 80kHz uses 8 phases (22.5deg steps),

40kHz and below use 16 phases (11.25deg steps).

Parameters

  frequency_hz | Frequency context in Hz.
  phase_deg | Requested phase in degrees.

Freq FCGEN Phase Phase selector. lower other 0.. 11.25 ..168.75 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15 80kHz 0b0001 0.. 22.5 ..157.50 0,1,2,3,4,5,6,7 128kHz 0b0000 0.. 45.0 ..135 0,1,2,3

BIOZ_phase is a global variable representing current phase setting

For quadrature measurement we want phase at 0 and 90deg magnitude is sqrt(R_0^2 + R_90^2) phase is atan(R_90/R_0)

If we measure multiple phases we need to fit curve measured R(offset) = mag*cos(phase+offset)

## ◆ setBIOZSamplingRate()

void MAX30001G::setBIOZSamplingRate | ( | uint8_t | speed_select | ) |

Set BIOZ sample-rate selector.

0 approx 30 sps (25-32) depending on FMSTR

1 approx 60 sps (50-64) depending on FMSTR *

Parameters

  speed_select | 0 low-rate mode (25-32sps), 1 high-rate mode (50..64sps)

## ◆ setBIOZTestImpedance()

void MAX30001G::setBIOZTestImpedance | ( | bool | enable,
|  | bool | useHighResistance,
|  | bool | enableModulation,
|  | uint8_t | rnomValue,
|  | uint8_t | rmodValue,
|  | uint8_t | modFreq
| ) |  |

Configure BIOZ test impedance and optional modulation.

Parameters

  enable | True to enable test impedance.
  useHighResistance | True for high-resistance RNOM table.
  enableModulation | True to enable RMOD modulation.
  rnomValue | RNOM selector.
  rmodValue | RMOD selector.
  modFreq | Modulation frequency selector (0..3).

useHighResistance=true, rnomValue 0..3 -> 27k,108k,487k,1029k

0 00 = 27 kΩ

1 01 = 108 kΩ

2 10 = 487 kΩ

3 11 = 1029 kΩ

useHighResistance=false, rnomValue 0..7 -> 5k..625ohm

0 000 = 5 kΩ

1 001 = 2.5 kΩ

2 010 = 1.667 kΩ

3 011 = 1.25 kΩ

4 100 = 1 kΩ

5 101 = 0.833 kΩ

6 110 = 0.714 kΩ

7 111 = 0.625 kΩ

enableModulation=true enables RMOD with rmodValue and modFreq.

For low resistance values between 625Ω and 5kΩ, the resistance can be modulated.

Resistance will switch between RNOM (resistance) and (RNOM - RMOD) at the selected modulation rate.

- rmodValue: Modulated resistance setting (0 to 7, RMOD). Only applicable when using low resistance.

- modFreq: resistance modulation frequency (0 to 3). Only applicable when using low resistance.

0=4Hz, 1=1Hz, 2=0.25Hz, 3=0.0625Hz

BMUX_RNOM[2:0] BMUX_RMOD[2:0] NOMINAL RESISTANCE (Ω) MODULATED RESISTANCE (mΩ)

000 000 5000 2960

001 980.5

010 247.5

1xx none

001 000 2500 740.4

001 245.2

010 61.9

1xx none

010 000 1667 329.1

001 109.0

010 27.5

1xx none

011 000 1250 185.1

001 61.3

010 none

1xx none

100 000 1000 118.5

001 39.2

010 none

1xx none

101 000 833 82.3

001 27.2

010 none

1xx none

110 000 714 60.5

001 20.0

010 none

1xx none

111 000 625 46.3

001 15.3

010 none

1xx none

## ◆ setDefaultBIOZTestImpedance()

void MAX30001G::setDefaultBIOZTestImpedance | ( | void |  | ) |

Apply default internal BIOZ test impedance settings.

## ◆ setDefaultBIOZTestSignal()

void MAX30001G::setDefaultBIOZTestSignal | ( | void |  | ) |

Apply default BIOZ voltage calibration signal settings.

## ◆ setDefaultECGandBIOZTestSignal()

void MAX30001G::setDefaultECGandBIOZTestSignal | ( | void |  | ) |

Apply default voltage calibration settings to ECG and BIOZ.

## ◆ setDefaultECGTestSignal()

void MAX30001G::setDefaultECGTestSignal | ( | void |  | ) |

Apply default ECG voltage calibration signal settings.

## ◆ setDefaultInterruptClearing()

void MAX30001G::setDefaultInterruptClearing | ( | void |  | ) |

Configure default interrupt-clear, clears on RR read, fast recovery read, and sample read.

## ◆ setDefaultNoBIOZTestImpedance()

void MAX30001G::setDefaultNoBIOZTestImpedance | ( | void |  | ) |

Disable internal BIOZ test impedance path.

## ◆ setDefaultNoRtoR()

void MAX30001G::setDefaultNoRtoR | ( | void |  | ) |

Apply default RTOR settings with RTOR disabled.

Default RtoR parameters are:

- enable: true

- ptsf: 0b0011 (4/16)

This is the fraction of the Peak Average value used in the Threshold computation.

- ptsf: 0b0101 (6/16) is also a common value for the threshold.

- pavg: 0b10 (8) default but 2 might also be used, how many past peak values are used to update peak thershold

This is the weighting factor for the current R-to-R peak observation vs. past peak observations when determining peak thresholds.

- gain: 0b1111 (Auto-Scale)

- wndw: 0b0011 12xRTOR_RES (~96ms)

- hoff: 0b100000 (32)

- ravg: 0b10 (8)

- rhsf: 0b100 (4/8)

## ◆ setDefaultNoTestSignal()

void MAX30001G::setDefaultNoTestSignal | ( | void |  | ) |

Disable ECG/BIOZ voltage calibration source routing.

## ◆ setDefaultRtoR()

void MAX30001G::setDefaultRtoR | ( | void |  | ) |

Apply default RTOR settings and enable RTOR detection.

## ◆ setECGAutoRecovery()

void MAX30001G::setECGAutoRecovery | ( | int | threshold_voltage | ) |

Enable automatic ECG fast-recovery mode.

Parameters

  threshold_voltage | Threshold in mV used to compute FAST_TH.

## ◆ setECGfilter()

void MAX30001G::setECGfilter | ( | uint8_t | lpf,
|  | uint8_t | hpf
| ) |  |

Configure ECG digital filters.

digital lpf for the AFE

0 bypass ~ 0 Hz

1 low ~ 40 Hz

2 medium ~100 Hz

3 high ~150 Hz

digital hpf for the AFE

0 bypass * default for all speeds

1 0.5 Hz

fixed external analog HPF on C_HPF:

0.1 uF 5.00 Hz (best motion artifact suppression)

1.0 uF 0.50 Hz

10.0 uF 0.05 Hz (MediBrick, highest signal quality preference)

Parameters

  lpf | LPF selector (0 bypass, 1 low, 2 medium, 3 high).
  hpf | HPF selector (0 bypass, 1 enable 0.5Hz class).

## ◆ setECGgain()

void MAX30001G::setECGgain | ( | uint8_t | gain | ) |

Set ECG PGA gain.

0 20 V/V

1 40 V/V

2 80 V/V * default

3 160 V/V

Parameters

  gain | Gain selector (0..3 => 20, 40, 80, 160 V/V).

## ◆ setECGLeadPolarity()

void MAX30001G::setECGLeadPolarity | ( | bool | inverted,
|  | bool | open
| ) |  |

Configure ECG polarity and input switch state.

Parameters

  inverted | True to swap ECG polarity.
  open | True to open inputs for calibration routing.

## ◆ setECGNormalRecovery()

void MAX30001G::setECGNormalRecovery | ( | void |  | ) |

## ◆ setECGSamplingRate()

void MAX30001G::setECGSamplingRate | ( | uint8_t | ECG | ) |

Set ECG sample-rate selector.

0 low ~125sps

1 medium ~256sps

2 high ~512sps * default

Parameters

  ECG | Rate selector (0 low, 1 medium, 2 high; constrained by FMSTR).

## ◆ setFIFOInterruptThreshold()

void MAX30001G::setFIFOInterruptThreshold | ( | uint8_t | ecg,
|  | uint8_t | bioz
| ) |  |

Set FIFO threshold that triggers ECG/BIOZ FIFO interrupts.

Parameters

  ecg | ECG threshold in samples (device supports 1..32).
  bioz | BIOZ threshold in samples (device supports 1..8).

## ◆ setFMSTR()

void MAX30001G::setFMSTR | ( | uint8_t | fmstr | ) |

Set master clock selector and recompute timing globals.

0 0b00 = 32768 Hz = FCLK

1 0b01 = 32000 Hz = FCLK*625/640

2 0b10 = 32000 Hz = FCLK*625/640

3 0b11 = 31968.78 Hz = FCLK*640/656

Parameters

  fmstr | FMSTR selector (0..3)(32768, 32000, 32000, 31968.78 Hz)

## ◆ setInterrupt1()

bool MAX30001G::setInterrupt1 | ( | bool | ecg,
|  | bool | bioz,
|  | bool | rtor,
|  | bool | leadon,
|  | bool | leadoff,
|  | bool | bioz_fourwire = `false`
| ) |  |
| inline

Configure interrupt line INT1 event enables.

Parameters

  ecg | Enable ECG-related interrupt bits.
  bioz | Enable BIOZ-related interrupt bits.
  rtor | Enable RTOR interrupt bit.
  leadon | Enable lead-on interrupt bit.
  leadoff | Enable lead-off interrupt bit.
  bioz_fourwire | Enable 4-wire BIOZ current monitor interrupt behavior.

Returns
  True when register write/verify succeeds.

## ◆ setInterrupt2()

bool MAX30001G::setInterrupt2 | ( | bool | ecg,
|  | bool | bioz,
|  | bool | rtor,
|  | bool | leadon,
|  | bool | leadoff,
|  | bool | bioz_fourwire = `false`
| ) |  |
| inline

Configure interrupt line INT2 event enables.

Parameters

  ecg | Enable ECG-related interrupt bits.
  bioz | Enable BIOZ-related interrupt bits.
  rtor | Enable RTOR interrupt bit.
  leadon | Enable lead-on interrupt bit.
  leadoff | Enable lead-off interrupt bit.
  bioz_fourwire | Enable 4-wire BIOZ current monitor interrupt behavior.

Returns
  True when register write/verify succeeds.

## ◆ setInterruptAggregateCallback()

bool MAX30001G::setInterruptAggregateCallback | ( | InterruptCallback | cb,
|  | void * | context = `nullptr`,
|  | uint32_t | statusMask = `0x00FFFFFFUL`
| ) |  |

Register aggregate callback invoked for status bits matching a mask.

Parameters

  cb | Callback function pointer.
  context | User context pointer passed to callback.
  statusMask | STATUS bit mask used for callback gating.

Returns
  True when registration succeeds.

## ◆ setInterruptEventCallback()

bool MAX30001G::setInterruptEventCallback | ( | InterruptEvent | event,
|  | InterruptCallback | cb,
|  | void * | context = `nullptr`
| ) |  |

Register callback for one specific interrupt event.

device - MAX30001G instance

status - STATUS register snapshot captured by serviceAllInterrupts()

context - user pointer passed at registration time

event - one value from InterruptEvent (for example IRQ_ECG_FIFO, IRQ_BIOZ_FIFO, IRQ_RTOR).

Parameters

  event | Interrupt event selector.
  cb | Callback function pointer.
  context | User context pointer passed to callback.

Returns
  True when registration succeeds.

## ◆ setLeadsBias()

void MAX30001G::setLeadsBias | ( | bool | enable,
|  | uint8_t | resistance
| ) |  |

Configure lead-bias mode and resistance.

resistance:

0 use external lead bias (in BIOZ mode, only available for high current mode)

>=150 internal lead bias 200M Ohm

> 75 internal lead bias 100M Ohm default

else internal lead bias 50M Ohm

Parameters

  enable | True to enable lead-bias path.
  resistance | Resistance selector value (mapped to internal/external options).

## ◆ setLeadsOffDetection()

void MAX30001G::setLeadsOffDetection | ( | bool | enable,
|  | bool | bioz_4,
|  | uint8_t | electrode_impedance
| ) |  |

Configure lead-off detection behavior.

Configure leads off detection for the ECG or BioZ channels.

The correct leads off detection features are automaticaly enabled (DC, Current and AC leads off)

Before running this routine

- Make sure that ecg or bioz is active.

- Lead polarity is set

electrode_impedance:

- 0-2, 2-4, 4-10, 10-20, >20 MOhm

- used to determine current magnitude, wet electrodes need higher current for lead-off detection
  Parameters

    enable | True to enable lead-off detection.
    bioz_4 | True for 4-wire BIOZ assumptions, false for 2-wire.
    electrode_impedance | Electrode impedance estimate in MOhm.

## ◆ setLeadsOnDetection()

void MAX30001G::setLeadsOnDetection | ( | bool | enable | ) |

Enable/disable ultra-low-power lead-on detection.

Lead on is used in low power mode to assert interrupt when leads are

attached so that the device can automatically power on

Parameters

  enable | True to enable ULP lead-on detection.

## ◆ setRtoR()

void MAX30001G::setRtoR | ( | bool | enable,
|  | uint8_t | ptsf,
|  | uint8_t | pavg,
|  | uint8_t | gain,
|  | uint8_t | wndw,
|  | uint8_t | hoff,
|  | uint8_t | ravg,
|  | uint8_t | rhsf
| ) |  |

Configure RTOR algorithm parameters.

ptsf: 0..15 maps to threshold scale 1/16..16/16.

pavg: 0..3 maps to peak averaging depth {2,4,8,16}.

gain: 0..15 maps to RTOR gain table (15 is auto-scale).

wndw: 0..11 valid QRS windows, 12..15 reserved.

hoff: 0..63 hold-off counts.

ravg: 0..3 maps to interval averaging depth {2,4,8,16}.

rhsf: 0..7 maps to dynamic hold-off scale 0/8..7/8.

Parameters

  enable | True to enable RTOR detection.
  ptsf | Peak threshold scaling factor selector (0..15).
  pavg | Peak averaging selector (0..3).
  gain | RTOR gain selector (0..15).
  wndw | QRS averaging window selector (0..11 valid, 12..15 reserved).
  hoff | Minimum hold-off selector (0..63).
  ravg | Interval averaging selector (0..3).
  rhsf | Dynamic hold-off scaling selector (0..7).

## ◆ setTestSignal()

void MAX30001G::setTestSignal | ( | bool | enableECGCalSignal,
|  | bool | enableBIOZCalSignal,
|  | bool | unipolar,
|  | bool | cal_vmag,
|  | uint8_t | freq,
|  | uint8_t | dutycycle
| ) |  |

Configure calibration voltage source and waveform settings.

freq (FCAL): 0..7 maps to FMSTR/{128,512,2048,8192,32768,131072,524288,2097152}.

Example at FMSTR=32768Hz: {256,64,16,4,1,0.25,0.0625,0.015625}Hz.

dutycycle: 1..99% valid, 50% uses the dedicated CALP_SEL path.

Parameters

  enableECGCalSignal | True to route VCAL to ECG path.
  enableBIOZCalSignal | True to route VCAL to BIOZ path.
  unipolar | True for unipolar waveform, false for bipolar waveform.
  cal_vmag | False for 0.25mV class, true for 0.5mV class.
  freq | FCAL selector (0..7).
  dutycycle | Duty cycle in percent (1..99, 50 uses dedicated mode).

## ◆ setupBIOZ()

void MAX30001G::setupBIOZ | ( | uint8_t | speed = `0`,
|  | uint8_t | gain = `1`,
|  | uint8_t | ahpf = `1`,
|  | uint8_t | dlpf = `1`,
|  | uint8_t | dhpf = `0`,
|  | uint32_t | frequency = `40000`,
|  | uint32_t | current = `8000`,
|  | float | phase = `0.0f`,
|  | bool | leadbias = `true`,
|  | bool | leadsoffdetect = `false`,
|  | bool | fourleads = `false`
| ) |  |

Configure a ready-to-use BIOZ profile.

speed: 0=low-rate (~25..32sps), 1=high-rate (~50..64sps).

gain: 0=10V/V, 1=20V/V, 2=40V/V, 3=80V/V.

ahpf: 0=60Hz, 1=150Hz, 2=500Hz, 3=1kHz, 4=2kHz, 5=4kHz, 6/7=bypass.

dlpf: 0=bypass, 1=~4Hz, 2=~8Hz, 3=~16Hz.

dhpf: 0=bypass, 1=0.05Hz, 2/3=0.5Hz class.

Parameters

  speed | BIOZ sample-rate selector (0 low, 1 high).
  gain | BIOZ gain selector (0..3 => 10, 20, 40, 80 V/V).
  ahpf | BIOZ analog HPF selector (0..7).
  dlpf | BIOZ digital LPF selector (0..3).
  dhpf | BIOZ digital HPF selector (0..3).
  frequency | Target modulation frequency in Hz (mapped to nearest valid FCGEN).
  current | Target drive current in nA (mapped/clamped to valid settings).
  phase | Demodulation phase offset in degrees.
  leadbias | True to enable lead-bias configuration in setup.
  leadsoffdetect | True to configure lead-off detection in setup.
  fourleads | True for 4-wire BIOZ assumptions, false for 2-wire.

## ◆ setupBIOZExternalImpedanceCalibration()

void MAX30001G::setupBIOZExternalImpedanceCalibration | ( | uint32_t | frequency = `40000`,
|  | float | phase = `0.0f`
| ) |  |

Configure external impedance calibration path.

Parameters

  frequency | BIOZ modulation frequency target in Hz.
  phase | Demodulation phase offset in degrees.

## ◆ setupBIOZImpedanceCalibration()

void MAX30001G::setupBIOZImpedanceCalibration | ( | uint8_t | speed = `0`,
|  | uint8_t | gain = `1`,
|  | uint8_t | ahpf = `1`,
|  | uint8_t | dlpf = `1`,
|  | uint8_t | dhpf = `0`,
|  | uint32_t | frequency = `40000`,
|  | uint32_t | current = `8000`,
|  | float | phase = `0.0f`,
|  | uint32_t | resistance = `5000`,
|  | uint8_t | modulation = `0`,
|  | uint8_t | modulation_frequency = `3`
| ) |  |

Configure internal BIOZ impedance calibration/test path.

speed: 0=low-rate (~25..32sps), 1=high-rate (~50..64sps).

gain: 0=10V/V, 1=20V/V, 2=40V/V, 3=80V/V.

ahpf: 0=60Hz, 1=150Hz, 2=500Hz, 3=1kHz, 4=2kHz, 5=4kHz, 6/7=bypass.

dlpf: 0=bypass, 1=~4Hz, 2=~8Hz, 3=~16Hz.

dhpf: 0=bypass, 1=0.05Hz, 2/3=0.5Hz class.

modulation: 0=unchopped+LPF, 1=chopped no-LPF, 2=chopped+LPF, 3=chopped+resistive-CM.

modulation_frequency: 0=4Hz, 1=1Hz, 2=0.25Hz, 3=0.0625Hz.

Parameters

  speed | BIOZ sample-rate selector (0..1).
  gain | BIOZ gain selector (0..3).
  ahpf | BIOZ analog HPF selector (0..7).
  dlpf | BIOZ digital LPF selector (0..3).
  dhpf | BIOZ digital HPF selector (0..3).
  frequency | BIOZ modulation frequency target in Hz.
  current | BIOZ drive current target in nA.
  phase | Demodulation phase offset in degrees.
  resistance | Nominal internal test impedance value.
  modulation | Calibration modulation mode selector.
  modulation_frequency | Calibration modulation frequency selector.

## ◆ setupBIOZScan() [1/2]

void MAX30001G::setupBIOZScan | ( | const BIOZScanConfig & | config = `BIOZScanConfig()`,
|  | bool | reuseCurrents = `false`
| ) |  |

Configure lifecycle-driven BIOZ scan flow.

This does not start scanning immediately. Call start(), then drive with update().

Parameters

  config | Scan configuration parameters.
  reuseCurrents | True to reuse previously optimized current profile.

## ◆ setupBIOZScan() [2/2]

void MAX30001G::setupBIOZScan | ( | uint8_t | avg,
|  | bool | fast,
|  | bool | fourleads,
|  | bool | fullRange
| ) |  |

Configure lifecycle-driven BIOZ scan flow.

This does not start scanning immediately. Call start(), then drive with update().

Parameters

  avg | BIOZ FIFO average depth used per point.
  fast | True for high-rate BIOZ sampling.
  fourleads | True for 4-wire BIOZ assumptions.
  fullRange | True to include lowest available frequency bins.

## ◆ setupBIOZSignalCalibration()

void MAX30001G::setupBIOZSignalCalibration | ( | uint8_t | speed = `0`,
|  | uint8_t | gain = `1`
| ) |  |

Configure BIOZ voltage calibration signal path.

speed: 0=low-rate (~25..32sps), 1=high-rate (~50..64sps).

gain: 0=10V/V, 1=20V/V, 2=40V/V, 3=80V/V.

Parameters

  speed | BIOZ sample-rate selector (0..1).
  gain | BIOZ gain selector (0..3).

## ◆ setupECG()

void MAX30001G::setupECG | ( | uint8_t | speed = `1`,
|  | uint8_t | gain = `2`,
|  | bool | threeleads = `true`
| ) |  |

Configure a ready-to-use ECG profile.

speed

0 ~125 sps

1 ~256 sps * default

2 ~512 sps

gain

0 20 V/V

1 40 V/V

2 80 V/V * default

3 160 V/V

three leads

true 3 lead ECG (with ground on RL or LL) * default

false 2 lead ECG (with RA and LA only), should use internal leads bias

Parameters

  speed | ECG sample-rate selector (0 low, 1 medium, 2 high).
  gain | ECG gain selector (0..3 => 20, 40, 80, 160 V/V).
  threeleads | True for 3-lead operation, false for 2-lead operation.

## ◆ setupECGandBIOZ()

void MAX30001G::setupECGandBIOZ | ( | uint8_t | ecg_speed = `1`,
|  | uint8_t | ecg_gain = `2`,
|  | bool | ecg_threeleads = `true`,
|  | uint8_t | bioz_speed = `0`,
|  | uint8_t | bioz_gain = `1`,
|  | uint8_t | bioz_dlpf = `1`,
|  | uint8_t | bioz_dhpf = `0`,
|  | uint32_t | bioz_frequency = `8000`,
|  | uint32_t | bioz_current = `8000`,
|  | float | bioz_phase = `0.0f`,
|  | bool | leadbias = `true`,
|  | bool | leadsoffdetect = `false`,
|  | bool | bioz_fourleads = `false`
| ) |  |

Configure simultaneous ECG and BIOZ operation.

ecg_speed: 0=~125sps, 1=~256sps, 2=~512sps.

ecg_gain: 0=20V/V, 1=40V/V, 2=80V/V, 3=160V/V.

bioz_speed: 0=~25..32sps, 1=~50..64sps.

bioz_gain: 0=10V/V, 1=20V/V, 2=40V/V, 3=80V/V.

bioz_dlpf: 0=bypass, 1=~4Hz, 2=~8Hz, 3=~16Hz.

bioz_dhpf: 0=bypass, 1=0.05Hz, 2/3=0.5Hz class.

Parameters

  ecg_speed | ECG sample-rate selector (0..2).
  ecg_gain | ECG gain selector (0..3).
  ecg_threeleads | True for 3-lead ECG mode.
  bioz_speed | BIOZ sample-rate selector (0..1).
  bioz_gain | BIOZ gain selector (0..3).
  bioz_dlpf | BIOZ digital LPF selector (0..3).
  bioz_dhpf | BIOZ digital HPF selector (0..3).
  bioz_frequency | BIOZ modulation frequency target in Hz.
  bioz_current | BIOZ drive current target in nA.
  bioz_phase | BIOZ phase offset target in degrees.
  leadbias | True to configure lead bias.
  leadsoffdetect | True to configure lead-off detection.
  bioz_fourleads | True for 4-wire BIOZ assumptions.

## ◆ setupECGSignalCalibration()

void MAX30001G::setupECGSignalCalibration | ( | uint8_t | speed = `1`,
|  | uint8_t | gain = `2`
| ) |  |

Configure ECG voltage calibration signal path.

speed: 0=~125sps, 1=~256sps, 2=~512sps.

gain: 0=20V/V, 1=40V/V, 2=80V/V, 3=160V/V.

Parameters

  speed | ECG sample-rate selector (0..2).
  gain | ECG gain selector (0..3).

## ◆ start()

void MAX30001G::start | ( | void |  | ) |

Start measurement engines according to the most recent setup profile.

## ◆ startBIOZScan()

void MAX30001G::startBIOZScan | ( | void |  | ) |

Start state-machine style BIOZ scan flow.

Arms non-blocking scan execution; each update() call advances scan steps.

## ◆ startECGManualRecovery()

void MAX30001G::startECGManualRecovery | ( | void |  | ) |

## ◆ stepBIOZScan()

void MAX30001G::stepBIOZScan | ( | void |  | ) |

Advance state-machine style BIOZ scan flow by one step.

Executes one non-blocking scan state transition per call.

## ◆ stop()

void MAX30001G::stop | ( | void |  | ) |

Stop active measurement engines.

## ◆ stopBIOZScan()

void MAX30001G::stopBIOZScan | ( | void |  | ) |

Stop state-machine style BIOZ scan flow.

Stops scan flow and powers down AFE engines.

## ◆ stopECGManualRecovery()

void MAX30001G::stopECGManualRecovery | ( | void |  | ) |

## ◆ swReset()

void MAX30001G::swReset | ( | void |  | ) |

## ◆ synch()

void MAX30001G::synch | ( | void |  | ) |

## ◆ update()

bool MAX30001G::update | ( | bool | reportRaw = `false` | ) |

Service pending IRQ work and drain enabled FIFOs.

Parameters

  reportRaw | True to keep raw ADC codes, false to convert to engineering units.

Returns
  True if update handled any interrupt/data/fault work.

## ◆ updateRaw()

bool MAX30001G::updateRaw | ( | void |  | ) |
| inline

Alias for raw-code update cycle.

Returns
  True if update handled any interrupt/data/fault work.

The documentation for this class was generated from the following files:

- src/max30001g.h
- src/max30001g.cpp
- src/max30001g_calibration.cpp
- src/max30001g_comm.cpp
- src/max30001g_configure_bioz.cpp
- src/max30001g_configure_ecg.cpp
- src/max30001g_configure_leads.cpp
- src/max30001g_configure_rtor.cpp
- src/max30001g_interrupt.cpp
- src/max30001g_readdata.cpp
- src/max30001g_regs.cpp
- src/max30001g_system.cpp