MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
HealthCheckResult Struct Reference

HealthCheckResult structure for storing health check results. More...

`#include <max30001g_typedefs.h>`

## Public Attributes
bool | fault_present
uint32_t | info_reg
bool | pll_unlocked
bool | spi_ok
uint32_t | status_reg

## Detailed Description

HealthCheckResult structure for storing health check results.

Contains status information about the device's operational state.

spi_ok indicates whether SPI communication appears functional.

info_reg and status_reg store the raw contents of the INFO and STATUS registers for debugging.

pll_unlocked indicates whether the PLL_UNLOCK status bit is set, which can affect timing and data validity.

fault_present indicates whether any fault conditions are currently active, which may require attention or indicate issues with the device or measurement setup.

## Member Data Documentation

## ◆ fault_present

bool HealthCheckResult::fault_present

## ◆ info_reg

uint32_t HealthCheckResult::info_reg

## ◆ pll_unlocked

bool HealthCheckResult::pll_unlocked

## ◆ spi_ok

bool HealthCheckResult::spi_ok

## ◆ status_reg

uint32_t HealthCheckResult::status_reg

The documentation for this struct was generated from the following file:

- src/max30001g_typedefs.h