MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_ecg_reg Union Reference

CNFG_ECG (0x15) page 51. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t dhpf: 1
uint32_t dlpf: 2
uint32_t gain: 2
uint32_t rate: 2
uint32_t reserved: 8
uint32_t reserved1: 12
uint32_t reserved2: 1
uint32_t reserved3: 4
} | bit

## Detailed Description

CNFG_ECG (0x15) page 51.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_ecg_reg::all

## ◆

struct { ... } max30001_cnfg_ecg_reg::bit

## ◆ dhpf

uint32_t max30001_cnfg_ecg_reg::dhpf

## ◆ dlpf

uint32_t max30001_cnfg_ecg_reg::dlpf

## ◆ gain

uint32_t max30001_cnfg_ecg_reg::gain

## ◆ rate

uint32_t max30001_cnfg_ecg_reg::rate

## ◆ reserved

uint32_t max30001_cnfg_ecg_reg::reserved

## ◆ reserved1

uint32_t max30001_cnfg_ecg_reg::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_ecg_reg::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_ecg_reg::reserved3

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h