UUtzinger_DRV8704 0.1.0 Arduino library for the DRV8704 dual H-bridge gate driver

DRV8704CurrentLimitResult Member List

This is the complete list of members for DRV8704CurrentLimitResult, including all inherited members.

achievableMaxCurrentAmps | DRV8704CurrentLimitResult |
ampsPerTorqueCount | DRV8704CurrentLimitResult |
appliedCurrentLimitAmpsA | DRV8704CurrentLimitResult |
appliedCurrentLimitAmpsB | DRV8704CurrentLimitResult |
DRV8704CurrentLimitResult() | DRV8704CurrentLimitResult | inline
enabled | DRV8704CurrentLimitResult |
preset | DRV8704CurrentLimitResult |
pwmFrequencyHz | DRV8704CurrentLimitResult |
referenceShuntOhms | DRV8704CurrentLimitResult |
requestedCurrentLimitAmps | DRV8704CurrentLimitResult |
selectedGain | DRV8704CurrentLimitResult |
shuntOhmsA | DRV8704CurrentLimitResult |
shuntOhmsB | DRV8704CurrentLimitResult |
torqueDac | DRV8704CurrentLimitResult |
valid | DRV8704CurrentLimitResult |