UUtzinger_DRV8704 0.1.0 Arduino library for the DRV8704 dual H-bridge gate driver

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:

C DRV8704 | Arduino-facing DRV8704 device driver class
C drv8704_blank_reg_t | BLANK register (0x03) view
C drv8704_ctrl_reg_t | CTRL register (0x00) view
C drv8704_decay_reg_t | DECAY register (0x04) view
C drv8704_drive_reg_t | DRIVE register (0x06) view
C drv8704_off_reg_t | OFF register (0x02) view
C drv8704_status_reg_t | STATUS register (0x07) view
C drv8704_torque_reg_t | TORQUE register (0x01) view
C DRV8704BridgeState | Reported direction and runtime mode of one bridge
C DRV8704Config | High-level DRV8704 configuration snapshot
C DRV8704CurrentLimitResult | Derived chip-global current-limit settings and per-bridge consequences
C DRV8704CurrentPresetConfig | Timing and decay recommendation associated with a current-mode preset
C DRV8704HealthCheck | Minimal transport/bring-up health result
C DRV8704Pins | Pin assignment bundle for a DRV8704 instance
C DRV8704PwmBackend | Abstract board-specific PWM backend used for DRV8704 bridge inputs
C DRV8704PwmCapability | Resolved platform PWM capabilities for the active backend
C DRV8704PwmConfig | Requested PWM generator settings
C DRV8704Status | Decoded device status and fault state
C GateDriveConfig | Gate-drive configuration group