Serial Wombat Arduino Library

Loading...
Searching...
No Matches
SerialWombatPulseTimer Member List

This is the complete list of members for SerialWombatPulseTimer, including all inherited members.

_pin | SerialWombatPin | protected
_pinMode | SerialWombatPin | protected
_sw | SerialWombatPin | protected
begin(uint8_t pin, SerialWombatPulseTimerUnits units=SW_PULSETIMER_uS, bool pullUpEnabled=false) | SerialWombatPulseTimer | inline
digitalRead() | SerialWombatPin | inline
digitalWrite(uint8_t val) | SerialWombatPin | inline
disable() | SerialWombatPin | inline
enableOpenDrain(bool enabled) | SerialWombatPin | inline
enablePulldown(bool enabled) | SerialWombatPin | inline
enablePullup(bool enabled) | SerialWombatPin | inline
forceDMA(bool enabled) | SerialWombatPin | inline
HighCounts | SerialWombatPulseTimer |
initPacketNoResponse(uint8_t packetNumber, uint8_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55, uint8_t param4=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0=0x55, uint8_t param1=0x55, uint8_t param2=0x55, uint8_t param3=0x55) | SerialWombatPin | inline
initPacketNoResponse(uint8_t packetNumber, uint16_t param0, uint16_t param1, uint8_t param2=0x55) | SerialWombatPin | inline
LowCounts | SerialWombatPulseTimer |
MeasurementOverflowOccurred | SerialWombatPulseTimer |
pin() | SerialWombatPin | inline
pinMode(uint8_t mode, bool pullDown=false, bool openDrain=false) | SerialWombatPin | inline
Pulses | SerialWombatPulseTimer |
readHighCounts() | SerialWombatPulseTimer | inline
readLowCounts() | SerialWombatPulseTimer | inline
readPublicData() | SerialWombatPin | inline
readPulses() | SerialWombatPulseTimer | inline
refresh() | SerialWombatPulseTimer | inline
refreshHighCountsLowCounts() | SerialWombatPulseTimer | inline
refreshHighCountsPulses() | SerialWombatPulseTimer | inline
SerialWombatPin(SerialWombatChip &serialWombatChip) | SerialWombatPin | inline
SerialWombatPin(SerialWombatChip &serialWombatChip, uint8_t pin) | SerialWombatPin | inline
SerialWombatPulseTimer(SerialWombatChip &serialWombat) | SerialWombatPulseTimer | inline
setPinNumberForTesting(uint8_t pin) | SerialWombatPin | inline
swPinModeNumber() | SerialWombatPin | inline
writePublicData(uint16_t value) | SerialWombatPin | inline