| ButtonToSwitch Library for Arduino v4.6.0 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
VdblMPBttn Class Referenceabstract

Abstract class, base to model Voidable DD-MPBs (VDD-MPB). More...

`#include <ButtonToSwitch.h>`

Inheritance diagram for VdblMPBttn:
[legend]
Collaboration diagram for VdblMPBttn:
[legend]

## Public Member Functions
| VdblMPBttn ()
| Default constructor.
| VdblMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0, const bool &isOnDisabled=false)
| Class constructor.
virtual | ~VdblMPBttn ()
| Default virtual destructor.
void | clrStatus (bool clrIsOn=true)
| See DbncdMPBttn::clrStatus(bool)
fncPtrType | getFnWhnTrnOffVdd ()
| Returns the function that is set to execute every time the object exits the Voided State.
fncPtrType | getFnWhnTrnOnVdd ()
| Returns the function that is set to execute every time the object enters the Voided or "Voided On" State.
bool | getFrcOtptLvlWhnVdd ()
| Returns the value of the frcOtptLvlWhnVdd attribute.
fncVdPtrPrmPtrType | getFVPPWhnTrnOffVdd ()
| Returns a pointer to a function that is set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.
void * | getFVPPWhnTrnOffVddArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOnVdd ()
| Returns a pointer to a function that is set to execute every time the object enters the Voided On State a.k.a. Voided State.
void * | getFVPPWhnTrnOnVddArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.
const bool | getIsVoided () const
| Returns the current value of the isVoided attribute flag.
bool | getStOnWhnOtpFrcd ()
| Returns the value of the frcOtptLvlWhnVdd attribute.
void | setFnWhnTrnOffVddPtr (void(*newFnWhnTrnOff)())
| Sets the function that will be called to execute every time the object's isVoided attribute flag is reset.
void | setFnWhnTrnOnVddPtr (void(*newFnWhnTrnOn)())
| Sets the function that will be called to execute every time the object's isVoided attribute flag is set.
void | setFVPPWhnTrnOffVdd (fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Voided Off State a.k.a. Not Voided State.
void | setFVPPWhnTrnOffVddArgPtr (void *newFVPPWhnTrnOffArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.
void | setFVPPWhnTrnOnVdd (fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Voided On State a.k.a. Voided State.
void | setFVPPWhnTrnOnVddArgPtr (void *newFVPPWhnTrnOnArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.
bool | setIsNotVoided ()
| Sets the value of the isVoided attribute flag to false.
bool | setIsVoided ()
| Sets the value of the isVoided attribute flag to true.
Public Member Functions inherited from DbncdDlydMPBttn
| DbncdDlydMPBttn ()
| Default constructor.
| DbncdDlydMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| DbncdDlydMPBttn (const DbncdDlydMPBttn &other)
| Copy constructor.
virtual | ~DbncdDlydMPBttn ()
| Class destructor.
bool | init (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| see DbncdMPBttn::init(const uint8_t, const bool, const bool, const unsigned long int)
void | setStrtDelay (const unsigned long int &newStrtDelay)
| Sets a new value to the "Start Delay" strtDelay attribute.
Public Member Functions inherited from DbncdMPBttn
| DbncdMPBttn ()
| Default class constructor.
| DbncdMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Class constructor.
| DbncdMPBttn (const DbncdMPBttn &other)
| Copy constructor.
virtual | ~DbncdMPBttn ()
| Default virtual destructor.
virtual bool | begin (const unsigned long int &pollDelayMs=_StdPollDelay)
| Attaches the instantiated object to a timer that monitors the input pins and updates the object status.
void | clrStatus (bool clrIsOn=true)
| Clears and resets flags, timers and counters modified through the object's signals processing.
void | disable ()
| Disables the input signal processing, ignoring the changes of its values.
void | enable ()
| Enables the input signal processing.
bool | end ()
| Detaches the object from the timer that monitors the input pins, compute and updates the object's status.
const unsigned long int | getCurDbncTime () const
| Returns the current debounce period time set for the object.
fncPtrType | getFnWhnTrnOff ()
| Returns the function that is set to execute every time the object enters the Off State.
fncPtrType | getFnWhnTrnOn ()
| Returns the function that is set to execute every time the object enters the On State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOff ()
| Returns a pointer to a function that is set to execute every time the object enters the Off State.
void * | getFVPPWhnTrnOffArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Off State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOn ()
| Returns a pointer to a function that is set to execute every time the object enters the On State.
void * | getFVPPWhnTrnOnArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the On State.
const bool | getIsEnabled () const
| Returns the value of the isEnabled attribute flag, indicating the Enabled or Disabled status of the object.
const bool | getIsOn () const
| Returns the value of the isOn attribute flag.
const bool | getIsOnDisabled () const
| Returns the value of the isOnDisabled attribute.
const unsigned long int | getLstPollTime ()
| Returns the time stamp of the last state update for the object.
const uint32_t | getOtptsSttsPkgd ()
| Returns the relevant attribute flags values for the object state encoded as a 32 bits value.
const bool | getOutputsChange () const
| Returns the value of the outputsChange attribute flag.
const unsigned long int | getPollPeriodMs ()
| Returns the poll period time setting attribute's value.
unsigned long int | getStrtDelay ()
| Returns the current value of strtDelay attribute.
bool | getUpdTmrAttchd ()
| Returns the value of the Attached to the update timer attribute.
bool | init (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Initializes an object instantiated by the default constructor.
bool | pause ()
| Pauses the software timer updating the computation of the object's internal flags value (object's state).
void | resetDbncTime ()
| Resets the debounce process time of the object to the value used at instantiation.
void | resetFda ()
| Resets the MPB behavior automaton to it's Initial or Start State
bool | resume ()
| Restarts the software timer updating the calculation of the object internal flags.
void | setBeginDisabled (const bool &newBeginDisabled=false)
| Sets the starting isDisabled state.
bool | setDbncTime (const unsigned long int &newDbncTime)
| Sets the debounce process time.
void | setFnWhnTrnOffPtr (void(*newFnWhnTrnOff)())
| Sets the function that will be called to execute every time the object enters the Off State.
void | setFnWhnTrnOnPtr (void(*newFnWhnTrnOn)())
| Sets the function that will be called to execute every time the object enters the On State.
void | setFVPPWhnTrnOff (fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Off State.
void | setFVPPWhnTrnOffArgPtr (void *newFVPPWhnTrnOffArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Off State.
void | setFVPPWhnTrnOn (fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the On State.
void | setFVPPWhnTrnOnArgPtr (void *newFVPPWhnTrnOnArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the On State.
void | setIsOnDisabled (const bool &newIsOnDisabled)
| Sets the value of the isOnDisabled attribute.
void | setOutputsChange (bool newOutputsChange)
| Sets the value of the attribute flag indicating if a change took place in any of the output attribute flags (IsOn included).

## Detailed Description

Abstract class, base to model Voidable DD-MPBs (VDD-MPB).

Voidable DD-MPBs are MPBs whose distinctive characteristic is that implement non-latching switches that while being pressed their state might change from On State to a Voided state due to different voiding conditions. Depending on the classes the voided state might be Voided & Off state, Voided & On state or Voided & Not enforced states. Those conditions to change to a voided state include -but are not limited to- the following conditions:

- pressing time
- external signals
- entering the On state

The mechanisms to "un-void" the MPB and return it to an operational state includes -but are not limited to- the following actions:

- releasing the MPBs
- receiving an external signal
- the reading of the isOn attribute flag status

The voiding conditions and the un-voiding mechanisms define the VDD-MPB subclasses.

## Constructor & Destructor Documentation

## ◆ VdblMPBttn()

VdblMPBttn::VdblMPBttn | ( | const uint8_t & | mpbttnPin,
|  | const bool & | pulledUp = true,
|  | const bool & | typeNO = true,
|  | const unsigned long int & | dbncTimeOrigSett = 0,
|  | const unsigned long int & | strtDelay = 0,
|  | const bool & | isOnDisabled = false )

Class constructor.

Parameters

  isOnDisabled | (Optional) Sets the instantiation value for the isOnDisabled flag attribute.

Note
  For the other parameters see DbncdDlydMPBttn(GPIO_TypeDef*, const uint16_t, const bool, const bool, const unsigned long int, const unsigned long int)

Here is the call graph for this function:

## Member Function Documentation

## ◆ getFnWhnTrnOffVdd()

fncPtrType VdblMPBttn::getFnWhnTrnOffVdd | ( |  | ) |

Returns the function that is set to execute every time the object exits the Voided State.

The function to be executed is an attribute that might be modified by the setFnWhnTrnOffVddPtr() method.

Returns
  A function pointer to the function set to execute every time the object enters the Unvoided or "Voieded Off" State.

Return values

  nullptr | if there is no function set to execute when the object enters the Unvoided (or "Voided Off") State.

## ◆ getFnWhnTrnOnVdd()

fncPtrType VdblMPBttn::getFnWhnTrnOnVdd | ( |  | ) |

Returns the function that is set to execute every time the object enters the Voided or "Voided On" State.

The function to be executed is an attribute that might be modified by the setFnWhnTrnOnVddPtr() method.

Returns
  A function pointer to the function set to execute every time the object enters the Voided (or "Voided On") State.

Return values

  nullptr | if there is no function set to execute when the object enters the Voided State.

## ◆ getFrcOtptLvlWhnVdd()

bool VdblMPBttn::getFrcOtptLvlWhnVdd | ( |  | ) |

Returns the value of the frcOtptLvlWhnVdd attribute.

The frcOtptLvlWhnVdd (Force Output Level When Voided) attribute configures the object to either keep it's isOn attribute flag current value when entering the voided state (false) or to force it to a specific isOn value (true).

Returns
  the current value of the frcOtptLvlWhnVdd attribute.

Note
  As of this version of the library no VdblMPBttn class or subclasses make use of the frcOtptLvlWhnVdd attribute, their inclusion is "New Features Under Development" related to the refactoring of binary states to Non-binary states.

## ◆ getFVPPWhnTrnOffVdd()

fncVdPtrPrmPtrType VdblMPBttn::getFVPPWhnTrnOffVdd | ( |  | ) |

Returns a pointer to a function that is set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

The pointer is one to a function with the signature void (fncPtr*) (void*) to allow for passing a void* argument to the function.

Returns
  fncVdPtrPrmPtrType The pointer to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

Return values

  nullptr | if there is no function with the described signature set to execute when the object enters the Voided Off State a.k.a. Not Voided State.

## ◆ getFVPPWhnTrnOffVddArgPtr()

void * VdblMPBttn::getFVPPWhnTrnOffVddArgPtr | ( |  | ) |

Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

Returns
  void* Pointer to the argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

## ◆ getFVPPWhnTrnOnVdd()

fncVdPtrPrmPtrType VdblMPBttn::getFVPPWhnTrnOnVdd | ( |  | ) |

Returns a pointer to a function that is set to execute every time the object enters the Voided On State a.k.a. Voided State.

The pointer is one to a function with the signature void (fncPtr*) (void*) to allow for passing a void* argument to the function.

Returns
  fncVdPtrPrmPtrType The pointer to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.

Return values

  nullptr | if there is no function with the described signature set to execute when the object enters the Voided On State a.k.a. Voided State.

## ◆ getFVPPWhnTrnOnVddArgPtr()

void * VdblMPBttn::getFVPPWhnTrnOnVddArgPtr | ( |  | ) |

Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.

Returns
  void* Pointer to the argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.

## ◆ getIsVoided()

const bool VdblMPBttn::getIsVoided | ( |  | ) | const

Returns the current value of the isVoided attribute flag.

Returns
  The value of the flag.

Return values

  true | The object is in voided state
  false | The object is in not voided state

## ◆ getStOnWhnOtpFrcd()

bool VdblMPBttn::getStOnWhnOtpFrcd | ( |  | ) |

Returns the value of the frcOtptLvlWhnVdd attribute.

The frcOtptLvlWhnVdd (Force Output Level When Voided) attribute configures the object to either keep it's isOn attribute flag current value when entering the voided state (false) or to force it to a specific isOn value (true).

If the object is set to force to a specific isOn value (true), the forced value to be set will be determined by the stOnWhnOtptFrcd attribute.

Returns
  the current value of the frcOtptLvlWhnVdd attribute.

Note
  As of this version of the library no VdblMPBttn class or subclasses make use of the frcOtptLvlWhnVdd attribute, their inclusion is "New Features Under Development" related to the refactoring of binary states to Non-binary states.

## ◆ setFnWhnTrnOffVddPtr()

void VdblMPBttn::setFnWhnTrnOffVddPtr | ( | void(* | newFnWhnTrnOff )() | ) |

Sets the function that will be called to execute every time the object's isVoided attribute flag is reset.

The function to be executed must be of the form void (*newFnWhnTrnOff)(), meaning it must take no arguments and must return no value, it will be executed only once by the object (recursion must be handled with the usual precautions). When instantiated the attribute value is set to nullptr.

Parameters

  newFnWhnTrnOff | Function pointer to the function intended to be called when the object's isVoided attribute flag is reset. Passing nullptr as parameter deactivates the function execution mechanism.

## ◆ setFnWhnTrnOnVddPtr()

void VdblMPBttn::setFnWhnTrnOnVddPtr | ( | void(* | newFnWhnTrnOn )() | ) |

Sets the function that will be called to execute every time the object's isVoided attribute flag is set.

The function to be executed must be of the form void (*newFnWhnTrnOn)(), meaning it must take no arguments and must return no value, it will be executed only once by the object (recursion must be handled with the usual precautions). When instantiated the attribute value is set to nullptr.

Parameters

  newFnWhnTrnOn | function pointer to the function intended to be called when the object's isVoided is set. Passing nullptr as parameter deactivates the function execution mechanism.

## ◆ setFVPPWhnTrnOffVdd()

void VdblMPBttn::setFVPPWhnTrnOffVdd | ( | fncVdPtrPrmPtrType | newFVPPWhnTrnOff,
|  | void * | argPtr = nullptr )

Sets a function to be executed every time the object enters the Voided Off State a.k.a. Not Voided State.

The function to be executed must be of the form void (newFVPPWhnTrnOff)(void), meaning it must take a void pointer as argument and must return no value, it will be executed only once by the object (recursion must be handled with the usual precautions). When the object is instantiated the attribute value is set to nullptr.

Parameters

  newFVPPWhnTrnOff | Function pointer to the function intended to be called when the object enters the Voided Off State a.k.a. Not Voided State. Passing nullptr as parameter deactivates the function execution mechanism.
  argPtr | void pointer to an argument to be passed to the function when it is called.

## ◆ setFVPPWhnTrnOffVddArgPtr()

void VdblMPBttn::setFVPPWhnTrnOffVddArgPtr | ( | void * | newFVPPWhnTrnOffArgPtr | ) |

Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

The argument pointer is passed to the function set to execute when the object enters the Voided Off State a.k.a. Not Voided State. The pointer is set to nullptr when the object is instantiated.

Parameters

  newFVPPWhnTrnOffArgPtr | Pointer to an argument to be passed to the function set to execute every time the object enters the Voided Off State a.k.a. Not Voided State.

## ◆ setFVPPWhnTrnOnVdd()

void VdblMPBttn::setFVPPWhnTrnOnVdd | ( | fncVdPtrPrmPtrType | newFVPPWhnTrnOn,
|  | void * | argPtr = nullptr )

Sets a function to be executed every time the object enters the Voided On State a.k.a. Voided State.

The function to be executed must be of the form void (newFVPPWhnTrnOn)(void), meaning it must take a void pointer as argument and must return no value, it will be executed only once by the object (recursion must be handled with the usual precautions). When the object is instantiated the attribute value is set to nullptr.

Parameters

  newFVPPWhnTrnOn | Function pointer to the function intended to be called when the object enters the Voided On State a.k.a. Voided State. Passing nullptr as parameter deactivates the function execution mechanism.
  argPtr | void pointer to an argument to be passed to the function when it is called.

## ◆ setFVPPWhnTrnOnVddArgPtr()

void VdblMPBttn::setFVPPWhnTrnOnVddArgPtr | ( | void * | newFVPPWhnTrnOnArgPtr | ) |

Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.

The argument pointer is passed to the function set to execute when the object enters the Voided On State a.k.a. Voided State. The pointer is set to nullptr when the object is instantiated.

Parameters

  newFVPPWhnTrnOnArgPtr | Pointer to an argument to be passed to the function set to execute every time the object enters the Voided On State a.k.a. Voided State.

## ◆ setIsNotVoided()

bool VdblMPBttn::setIsNotVoided | ( |  | ) |

Sets the value of the isVoided attribute flag to false.

Warning
  The value of the isVoided attribute flag is computed as a result of the current state of the instantiated object, considering the inputs and embedded simulated behavior.
  - Arbitrarily setting a value to the isVoided attribute flag might affect the normal behavior path for the object.
  - The attribute flag value might return to it's natural value when the behavior imposes the change.
  - The use of this method must be limited to certain states and conditions of the object, being the most suitable situation while the object is in Disabled state: If the application development requires the isVoided attribute flag to be in a specific value, this method and the setIsVoided() method are the required tools.

Return values

  true |

Here is the caller graph for this function:

## ◆ setIsVoided()

bool VdblMPBttn::setIsVoided | ( |  | ) |

Sets the value of the isVoided attribute flag to true.

Warning
  See the Warnings for setIsNotVoided()

Return values

  true |