| ButtonToSwitch Library for Arduino v4.6.0 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
DDlydDALtchMPBttn Class Reference

Models a Debounced Delayed Double Action Latched MPB combo switch (Debounced Delayed DALDD-MPB - DD-DALDD-MPB) More...

`#include <ButtonToSwitch.h>`

Inheritance diagram for DDlydDALtchMPBttn:
[legend]
Collaboration diagram for DDlydDALtchMPBttn:
[legend]

## Public Member Functions
| DDlydDALtchMPBttn ()
| Default class constructor.
| DDlydDALtchMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| ~DDlydDALtchMPBttn ()
| Class virtual destructor.
void | clrStatus (bool clrIsOn=true)
| See DbncddMPBttn::clrStatus(bool)
Public Member Functions inherited from DblActnLtchMPBttn
| DblActnLtchMPBttn ()
| Abstract Class default constructor.
| DblActnLtchMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Abstract Class constructor.
| ~DblActnLtchMPBttn ()
| Virtual destructor.
virtual bool | begin (const unsigned long int &pollDelayMs=_StdPollDelay)
| See DbncdMPBttn::begin(const unsigned long int)
void | clrStatus (bool clrIsOn=true)
| See DbncddMPBttn::clrStatus(bool)
fncPtrType | getFnWhnTrnOffScndry ()
| returns the function that is set to execute every time the object enters the Secondary Off State.
fncPtrType | getFnWhnTrnOnScndry ()
| Returns the function that is set to execute every time the object enters the Secondary On State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOffScndry ()
| Returns a pointer to a function that is set to execute every time the object enters the Secondary Mode Off State.
void * | getFVPPWhnTrnOffScndryArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Secondary Mode Off State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOnScndry ()
| Returns a pointer to a function that is set to execute every time the object enters the Secondary Mode On State.
void * | getFVPPWhnTrnOnScndryArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Secondary Mode On State.
bool | getIsOnScndry ()
| Returns the current value of the isOnScndry attribute flag.
unsigned long | getScndModActvDly ()
| Returns the current value of the scndModActvDly class attribute.
void | setFnWhnTrnOffScndryPtr (void(*newFnWhnTrnOff)())
| Sets the function that will be called to execute every time the object enters the Secondary Off State.
void | setFnWhnTrnOnScndryPtr (void(*newFnWhnTrnOn)())
| Sets the function that will be called to execute every time the object enters the Secondary On State.
void | setFVPPWhnTrnOffScndry (fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Secondary Mode Off State.
void | setFVPPWhnTrnOffScndryArgPtr (void *newFVPPWhnTrnOffArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Secondary Mode Off State.
void | setFVPPWhnTrnOnScndry (fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Secondary Mode On State.
void | setFVPPWhnTrnOnScndryArgPtr (void *newFVPPWhnTrnOnArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Secondary Mode On State.
bool | setScndModActvDly (const unsigned long &newVal)
| Sets a new value for the scndModActvDly class attribute.
Public Member Functions inherited from LtchMPBttn
| LtchMPBttn ()
| Default constructor.
| LtchMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| LtchMPBttn (const LtchMPBttn &other)
| Copy constructor.
virtual | ~LtchMPBttn ()
| Class virtual destructor.
void | clrStatus (bool clrIsOn=true)
| See DbncdMPBttn::clrStatus(bool)
const bool | getIsLatched () const
| Returns the value of the isLatched attribute flag, indicating the Latched or Unlatched condition of the object.
bool | getTrnOffASAP ()
| Returns the value of the trnOffASAP attribute flag.
const bool | getUnlatchPend () const
| Returns the value of the "Valid Unlatch Pending" attribute.
const bool | getUnlatchRlsPend () const
| Returns the value of the "Valid Unlatch Release Pending" attribute.
void | setTrnOffASAP (const bool &newVal)
| Sets the value of the trnOffASAP attribute.
void | setUnlatchPend (const bool &newVal)
| Sets the value of the "Valid Unlatch Pending" attribute.
void | setUnlatchRlsPend (const bool &newVal)
| Sets the value of the "Valid Unlatch Release Pending" attribute.
bool | unlatch ()
| Sets the values of the flags needed to unlatch a latched MPB.
Public Member Functions inherited from DbncdDlydMPBttn
| DbncdDlydMPBttn ()
| Default constructor.
| DbncdDlydMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| Class constructor.
| DbncdDlydMPBttn (const DbncdDlydMPBttn &other)
| Copy constructor.
virtual | ~DbncdDlydMPBttn ()
| Class destructor.
bool | init (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0)
| see DbncdMPBttn::init(const uint8_t, const bool, const bool, const unsigned long int)
void | setStrtDelay (const unsigned long int &newStrtDelay)
| Sets a new value to the "Start Delay" strtDelay attribute.
Public Member Functions inherited from DbncdMPBttn
| DbncdMPBttn ()
| Default class constructor.
| DbncdMPBttn (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Class constructor.
| DbncdMPBttn (const DbncdMPBttn &other)
| Copy constructor.
virtual | ~DbncdMPBttn ()
| Default virtual destructor.
void | clrStatus (bool clrIsOn=true)
| Clears and resets flags, timers and counters modified through the object's signals processing.
void | disable ()
| Disables the input signal processing, ignoring the changes of its values.
void | enable ()
| Enables the input signal processing.
bool | end ()
| Detaches the object from the timer that monitors the input pins, compute and updates the object's status.
const unsigned long int | getCurDbncTime () const
| Returns the current debounce period time set for the object.
fncPtrType | getFnWhnTrnOff ()
| Returns the function that is set to execute every time the object enters the Off State.
fncPtrType | getFnWhnTrnOn ()
| Returns the function that is set to execute every time the object enters the On State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOff ()
| Returns a pointer to a function that is set to execute every time the object enters the Off State.
void * | getFVPPWhnTrnOffArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the Off State.
fncVdPtrPrmPtrType | getFVPPWhnTrnOn ()
| Returns a pointer to a function that is set to execute every time the object enters the On State.
void * | getFVPPWhnTrnOnArgPtr ()
| Returns a pointer to the argument to be passed to the function set to execute every time the object enters the On State.
const bool | getIsEnabled () const
| Returns the value of the isEnabled attribute flag, indicating the Enabled or Disabled status of the object.
const bool | getIsOn () const
| Returns the value of the isOn attribute flag.
const bool | getIsOnDisabled () const
| Returns the value of the isOnDisabled attribute.
const unsigned long int | getLstPollTime ()
| Returns the time stamp of the last state update for the object.
const uint32_t | getOtptsSttsPkgd ()
| Returns the relevant attribute flags values for the object state encoded as a 32 bits value.
const bool | getOutputsChange () const
| Returns the value of the outputsChange attribute flag.
const unsigned long int | getPollPeriodMs ()
| Returns the poll period time setting attribute's value.
unsigned long int | getStrtDelay ()
| Returns the current value of strtDelay attribute.
bool | getUpdTmrAttchd ()
| Returns the value of the Attached to the update timer attribute.
bool | init (const uint8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0)
| Initializes an object instantiated by the default constructor.
bool | pause ()
| Pauses the software timer updating the computation of the object's internal flags value (object's state).
void | resetDbncTime ()
| Resets the debounce process time of the object to the value used at instantiation.
void | resetFda ()
| Resets the MPB behavior automaton to it's Initial or Start State
bool | resume ()
| Restarts the software timer updating the calculation of the object internal flags.
void | setBeginDisabled (const bool &newBeginDisabled=false)
| Sets the starting isDisabled state.
bool | setDbncTime (const unsigned long int &newDbncTime)
| Sets the debounce process time.
void | setFnWhnTrnOffPtr (void(*newFnWhnTrnOff)())
| Sets the function that will be called to execute every time the object enters the Off State.
void | setFnWhnTrnOnPtr (void(*newFnWhnTrnOn)())
| Sets the function that will be called to execute every time the object enters the On State.
void | setFVPPWhnTrnOff (fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the Off State.
void | setFVPPWhnTrnOffArgPtr (void *newFVPPWhnTrnOffArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the Off State.
void | setFVPPWhnTrnOn (fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr)
| Sets a function to be executed every time the object enters the On State.
void | setFVPPWhnTrnOnArgPtr (void *newFVPPWhnTrnOnArgPtr)
| Sets a pointer to an argument to be passed to the function set to execute every time the object enters the On State.
void | setIsOnDisabled (const bool &newIsOnDisabled)
| Sets the value of the isOnDisabled attribute.
void | setOutputsChange (bool newOutputsChange)
| Sets the value of the attribute flag indicating if a change took place in any of the output attribute flags (IsOn included).

## Detailed Description

Models a Debounced Delayed Double Action Latched MPB combo switch (Debounced Delayed DALDD-MPB - DD-DALDD-MPB)

This is a subclass of the DALDD-MPB whose secondary behavior is that of a DbncdDlydMPBttn (DD-MPB), that implies that:

- While on the 1.state (Off-Off), a short press will activate only the regular main On state 2. (On-Off).
- While on the 1.state (Off-Off), a long press will activate both the regular main On state and the secondary On state simultaneously 3. (On-On). When releasing the MPB the switch will stay in the main On state 2. (On-Off). While in the 2. state (On-Off), a short press will set the switch to the 1. state (Off-Off) While in the 2. state (On-Off), a long press will set the switch to the 3. state (On-On), until the releasing of the MPB, returning the switch to the main On state 2. (On-Off).

class DDlydDALtchMPBttn

## Constructor & Destructor Documentation

## ◆ DDlydDALtchMPBttn()

DDlydDALtchMPBttn::DDlydDALtchMPBttn | ( | const uint8_t & | mpbttnPin,
|  | const bool & | pulledUp = true,
|  | const bool & | typeNO = true,
|  | const unsigned long int & | dbncTimeOrigSett = 0,
|  | const unsigned long int & | strtDelay = 0 )

Class constructor.

Note
  For parameters see DbncdDlydMPBttn(const uint8_t, const bool, const bool, const unsigned long int, const unsigned long int)

Here is the call graph for this function: