| ButtonToSwitch Library for ESP32 (Arduino) v4.6.1 A library that provides elaborated switch mechanism behavior simulation for digital signals inputs

Loading...
Searching...
No Matches
DblActnLtchMPBttn Member List

This is the complete list of members for DblActnLtchMPBttn, including all inherited members.

begin(const unsigned long int &pollDelayMs=_StdPollDelay) | DblActnLtchMPBttn | virtual
clrStatus(bool clrIsOn=true) | DblActnLtchMPBttn |
DblActnLtchMPBttn() | DblActnLtchMPBttn |
DblActnLtchMPBttn(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0) | DblActnLtchMPBttn |
DbncdDlydMPBttn() | DbncdDlydMPBttn |
DbncdDlydMPBttn(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0) | DbncdDlydMPBttn |
DbncdDlydMPBttn(const DbncdDlydMPBttn &other) | DbncdDlydMPBttn |
DbncdMPBttn() | DbncdMPBttn |
DbncdMPBttn(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0) | DbncdMPBttn |
DbncdMPBttn(const DbncdMPBttn &other) | DbncdMPBttn |
disable() | DbncdMPBttn |
enable() | DbncdMPBttn |
end() | DbncdMPBttn |
getCurDbncTime() const | DbncdMPBttn |
getFnWhnTrnOff() | DbncdMPBttn |
getFnWhnTrnOffScndry() | DblActnLtchMPBttn |
getFnWhnTrnOn() | DbncdMPBttn |
getFnWhnTrnOnScndry() | DblActnLtchMPBttn |
getFVPPWhnTrnOff() | DbncdMPBttn |
getFVPPWhnTrnOffArgPtr() | DbncdMPBttn |
getFVPPWhnTrnOffScndry() | DblActnLtchMPBttn |
getFVPPWhnTrnOffScndryArgPtr() | DblActnLtchMPBttn |
getFVPPWhnTrnOn() | DbncdMPBttn |
getFVPPWhnTrnOnArgPtr() | DbncdMPBttn |
getFVPPWhnTrnOnScndry() | DblActnLtchMPBttn |
getFVPPWhnTrnOnScndryArgPtr() | DblActnLtchMPBttn |
getIsEnabled() const | DbncdMPBttn |
getIsLatched() const | LtchMPBttn |
getIsOn() const | DbncdMPBttn |
getIsOnDisabled() const | DbncdMPBttn |
getIsOnScndry() | DblActnLtchMPBttn |
getMpbInstnc() const | DbncdMPBttn |
getOtptsSttsPkgd() | DbncdMPBttn |
getOutputsChange() const | DbncdMPBttn |
getScndModActvDly() | DblActnLtchMPBttn |
getStrtDelay() | DbncdMPBttn |
getTaskToNotify() const | DbncdMPBttn |
getTaskWhileOn() | DbncdMPBttn |
getTaskWhileOnScndry() | DblActnLtchMPBttn |
getTrnOffASAP() | LtchMPBttn |
getUnlatchPend() const | LtchMPBttn |
getUnlatchRlsPend() const | LtchMPBttn |
init(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0) | DbncdDlydMPBttn |
DbncdMPBttn::init(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0) | DbncdMPBttn |
LtchMPBttn() | LtchMPBttn |
LtchMPBttn(const int8_t &mpbttnPin, const bool &pulledUp=true, const bool &typeNO=true, const unsigned long int &dbncTimeOrigSett=0, const unsigned long int &strtDelay=0) | LtchMPBttn |
LtchMPBttn(const LtchMPBttn &other) | LtchMPBttn |
pause() | DbncdMPBttn |
resetDbncTime() | DbncdMPBttn |
resetFda() | DbncdMPBttn |
resume() | DbncdMPBttn |
setBeginDisabled(const bool &newBeginDisabled=false) | DbncdMPBttn |
setDbncTime(const unsigned long int &newDbncTime) | DbncdMPBttn |
setFnWhnTrnOffPtr(fncPtrType newFnWhnTrnOff) | DbncdMPBttn |
setFnWhnTrnOffScndryPtr(void(*newFnWhnTrnOff)()) | DblActnLtchMPBttn |
setFnWhnTrnOnPtr(fncPtrType newFnWhnTrnOn) | DbncdMPBttn |
setFnWhnTrnOnScndryPtr(void(*newFnWhnTrnOn)()) | DblActnLtchMPBttn |
setFVPPWhnTrnOff(fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr) | DbncdMPBttn |
setFVPPWhnTrnOffArgPtr(void *newFVPPWhnTrnOffArgPtr) | DbncdMPBttn |
setFVPPWhnTrnOffScndry(fncVdPtrPrmPtrType newFVPPWhnTrnOff, void *argPtr=nullptr) | DblActnLtchMPBttn |
setFVPPWhnTrnOffScndryArgPtr(void *newFVPPWhnTrnOffArgPtr) | DblActnLtchMPBttn |
setFVPPWhnTrnOn(fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr) | DbncdMPBttn |
setFVPPWhnTrnOnArgPtr(void *newFVPPWhnTrnOnArgPtr) | DbncdMPBttn |
setFVPPWhnTrnOnScndry(fncVdPtrPrmPtrType newFVPPWhnTrnOn, void *argPtr=nullptr) | DblActnLtchMPBttn |
setFVPPWhnTrnOnScndryArgPtr(void *newFVPPWhnTrnOnArgPtr) | DblActnLtchMPBttn |
setIsOnDisabled(const bool &newIsOnDisabled) | DbncdMPBttn |
setOutputsChange(bool newOutputsChange) | DbncdMPBttn |
setScndModActvDly(const unsigned long &newVal) | DblActnLtchMPBttn |
setStrtDelay(const unsigned long int &newStrtDelay) | DbncdDlydMPBttn |
setTaskToNotify(const TaskHandle_t &newTaskHandle) | DbncdMPBttn |
setTaskWhileOn(const TaskHandle_t &newTaskHandle) | DbncdMPBttn | virtual
setTaskWhileOnScndry(const TaskHandle_t &newTaskHandle) | DblActnLtchMPBttn |
setTrnOffASAP(const bool &newVal) | LtchMPBttn |
setUnlatchPend(const bool &newVal) | LtchMPBttn |
setUnlatchRlsPend(const bool &newVal) | LtchMPBttn |
unlatch() | LtchMPBttn |
~DblActnLtchMPBttn() | DblActnLtchMPBttn |
~DbncdDlydMPBttn() | DbncdDlydMPBttn | virtual
~DbncdMPBttn() | DbncdMPBttn | virtual
~LtchMPBttn() | LtchMPBttn | virtual