LORAWAN OTAA EBYTE EoRa-S3-900TB for PlatformIO
===    
Example to be used with PlatformIO. This example is to show how to connect to the Helium network or TTN by OTAA activation. It is written only for the EoRa-S3-900TB : ESP32-S3 + E22-900MM22S (SX1262) + OLED display.

See [E22 ESP32 example](../LORAWAN-OTAA-esp32-e22/) for configuration.