| SX126x-Arduino 2.0.1

Data Structures | Typedefs | Functions
RegionCommon.h File Reference

Region independent implementations which are common to all regions. More...

Go to the source code of this file.

## Data Structures
struct | sRegionCommonLinkAdrParams
struct | sRegionCommonLinkAdrReqVerifyParams
struct | sRegionCommonCalcBackOffParams

## Typedefs
typedef struct sRegionCommonLinkAdrParams | RegionCommonLinkAdrParams_t
typedef struct sRegionCommonLinkAdrReqVerifyParams | RegionCommonLinkAdrReqVerifyParams_t
typedef struct sRegionCommonCalcBackOffParams | RegionCommonCalcBackOffParams_t

## Functions
uint16_t | RegionCommonGetJoinDc (TimerTime_t elapsedTime)
| Calculates the join duty cycle. This is a generic function and valid for all regions. More...
uint8_t | RegionCommonValueInRange (int8_t value, int8_t min, int8_t max)
| Verifies, if a value is in a given range. This is a generic function and valid for all regions. More...
bool | RegionCommonChanVerifyDr (uint8_t nbChannels, uint16_t *channelsMask, int8_t dr, int8_t minDr, int8_t maxDr, ChannelParams_t *channels)
| Verifies, if a datarate is available on an active channel. This is a generic function and valid for all regions. More...
bool | RegionCommonChanDisable (uint16_t *channelsMask, uint8_t id, uint8_t maxChannels)
| Disables a channel in a given channels mask. This is a generic function and valid for all regions. More...
uint8_t | RegionCommonCountChannels (uint16_t *channelsMask, uint8_t startIdx, uint8_t stopIdx)
| Counts the number of active channels in a given channels mask. This is a generic function and valid for all regions. More...
void | RegionCommonChanMaskCopy (uint16_t *channelsMaskDest, uint16_t *channelsMaskSrc, uint8_t len)
| Copy a channels mask. This is a generic function and valid for all regions. More...
void | RegionCommonSetBandTxDone (bool joined, Band_t *band, TimerTime_t lastTxDone)
| Sets the last tx done property. This is a generic function and valid for all regions. More...
TimerTime_t | RegionCommonUpdateBandTimeOff (bool joined, bool dutyCycle, Band_t *bands, uint8_t nbBands)
| Updates the time-offs of the bands. This is a generic function and valid for all regions. More...
uint8_t | RegionCommonParseLinkAdrReq (uint8_t *payload, RegionCommonLinkAdrParams_t *parseLinkAdr)
| Parses the parameter of an LinkAdrRequest. This is a generic function and valid for all regions. More...
uint8_t | RegionCommonLinkAdrReqVerifyParams (RegionCommonLinkAdrReqVerifyParams_t *verifyParams, int8_t *dr, int8_t *txPow, uint8_t *nbRep)
| Verifies and updates the datarate, the TX power and the number of repetitions of a LinkAdrRequest. This depends on the configuration of ADR also. More...
double | RegionCommonComputeSymbolTimeLoRa (uint8_t phyDr, uint32_t bandwidth)
| Computes the symbol time for LoRa modulation. More...
double | RegionCommonComputeSymbolTimeFsk (uint8_t phyDr)
| Computes the symbol time for FSK modulation. More...
void | RegionCommonComputeRxWindowParameters (double tSymbol, uint8_t minRxSymbols, uint32_t rxError, uint32_t wakeUpTime, uint32_t *windowTimeout, int32_t *windowOffset)
| Computes the RX window timeout and the RX window offset. More...
int8_t | RegionCommonComputeTxPower (int8_t txPowerIndex, float maxEirp, float antennaGain)
| Computes the txPower, based on the max EIRP and the antenna gain. More...
void | RegionCommonCalcBackOff (RegionCommonCalcBackOffParams_t *calcBackOffParams)
| Calculates the duty cycle for the current band. More...

## Detailed Description

Region independent implementations which are common to all regions.

Copyright
  Revised BSD License, see file LICENSE.

______ _
/ _____) _ | |
( (____ _____ ____ _| |_ _____ ____| |__
\____ \| ___ | (_ _) ___ |/ ___) _ \
_____) ) ____| | | || |_| ____( (___| | | |
(______/|_____)_|_|_| \__)_____)\____)_| |_|
(C)2013 Semtech
___ _____ _ ___ _ _____ ___ ___ ___ ___
/ __|_ _/_\ / __| |/ / __/ _ \| _ \/ __| __|
\__ \ | |/ _ \ (__| ' <| _| (_) | / (__| _|
|___/ |_/_/ \_\___|_|\_\_| \___/|_|_\\___|___|
embedded.connectivity.solutions===============

Author
  Miguel Luis ( Semtech )
  Gregory Cristian ( Semtech )
  Daniel Jaeckle ( STACKFORCE )