## esp-fs-webserver
This example is a little bit more advanced respect to the [simpleServer](https://github.com/cotestatnt/esp-fs-webserver/tree/main/examples/simpleServer) example.

Basically is the same HTML code like simpleServer, but with the addition of a **WebSocket client** inside the webpage.

Off course, on the ESP MCU we will run also a **WebSocket server** together to the web server.

With the help of WebSocket technology, we can send message from server-to-clients or from client-to-server in a **full-duplex communication channels over a single TCP connection.**

In this very simple example is used only to push from ESP side a message (the NTP updated ESP system time) to the connected clients, just to show hot to setup a system like this.

![image](https://user-images.githubusercontent.com/27758688/151001497-6468b50f-d4cb-46e1-ab4c-4d7aca3883db.png)
