pfodParser 3.61.0 The pfodParser library is handles commands sent from the Android pfodApp, pfodApp supports WiFi, BLE, Bluetooth and SMS connections

pfodMAC.h
Go to the documentation of this file.
1 #ifndef pfodMAC_h
2 #define pfodMAC_h
9 /*
10 (c)2014-2017 Forward Computing and Control Pty. Ltd.
11 NSW Australia, www.forward.com.au
12 This code is not warranted to be fit for any purpose. You may only use it at your own risk.
13 This code may be freely used for both private and commercial use
14 Provide this copyright is maintained.
15 */
16
17 #include <Arduino.h>
18 #include "pfodStream.h"
19 #include "pfodEEPROM.h"
20
21 #define MAX_ELAPSED_TIME 0x7fffffff
22
23 class pfodMAC {
24 public:
25
26 pfodMAC();
27 boolean init(int eepromAddress); // if eepromAddress < 0 disable EEPROM use
28
35 static void resetPowerCycles(int eepromAddress = 0);
36
37 void setSecretKey(byte *key, int len);
38
39 void setDebugStream(Print* out);
40 boolean isValid(); // powercycles > 0
41 boolean isBigEndian(); // is 1 stored as 0x00000001 false for Atmel 8 bit micros
42 void noEEPROM(); // disable eeprom
43
44 unsigned int readSecretKey(byte* bRtn, int keyAdd); // returns 0 length if EEPROM disabled
45
46 // utility methods
47 uint8_t eeprom_read(int address); // always returns 0 if EEPROM disabled
48 static void eeprom_write(int address, uint8_t value); // does nothing if EEPROM disabled
49
50 // useful for debugging
51 void printBytesInHex(Print *out, const byte* b, size_t len);
52
68 boolean buildChallenge(byte* challengeBytes, uint32_t mS_sinceLastConnection);
69
70 void initHash(); // start a new hash by initializing with the secret key
71 void putByteToHash(byte b); // add a byte to the hash
72 void putBytesToHash(byte* b, int len); // add a byte array to the hash
73 void putLongToHash(uint32_t l); // add a long to the hash (in BigEndian format)
74 void finishHash(); // finish the hash and calculate the result
75 byte* getHashedResult(); // get pointer to the 8 byte result
76
77
85 boolean checkMsgHash(const byte* msgHash, uint16_t len);
86
87 void reverseBytes(byte *b, int len); // swap from order of bytes upto len, converts between Endians, Big to Little, Little to Big
88
89 const static uint8_t msgHashByteSize = 4; // number of byte in per msg hash
90 const static uint8_t challengeHashByteSize = 8; // number of bytes in challenge hash
91 const static uint8_t challengeByteSize = 8; // number of bytes in challenge
92 const static uint8_t PowerCyclesOffset; // == 0 offset to power cycles from eepromAddress
93 const static uint8_t KeyOffset; // offset to keyLen from eepromAddress, length (1 byte) comes first then key
94 const static uint8_t maxKeySize = 16; // max size of key 128 bits
95
96 private:
97 boolean initCalled; // set true after first init() call. Stops multiple calls to get readPowerCycles
98 boolean cmpToResult(const byte* response, uint16_t len);
99 int CHAP_EEPROM_Address; // set to -1 if eeprom disabled
100 Print *debugOut;
101 boolean disableEEPROM; // true if NO EEPROM or eepromAddress arg is < 0
102 const static uint8_t powerCycleSize; // sizeof(uint16_t)
103 const static uint8_t timerSize; // sizeof(uint32_t)
104 const static uint8_t counterSize; // int
105 uint16_t connectionCounter; // increment each connection
106 uint16_t powerCycles;
107 byte key[maxKeySize]; // the secret key after reading from EEPROM and expanding to 16 bytes
108 uint8_t keyLen; // 0 if no key, else 16 (after padding key with 0 if shorter)
109 boolean bigEndian; // true if bigEndian uC
110 uint8_t *hashChallenge(byte *challenge); // hashes challenge returns pointer to 8 byte result
111
120 uint16_t readPowerCycles(int powerCycleAdd);
121
122 };
123
124
125 #endif // pfodMAC_h
126
pfodMAC
Definition: pfodMAC.h:23
pfodMAC::buildChallenge
boolean buildChallenge(byte *challengeBytes, uint32_t mS_sinceLastConnection)
buildChallenge – NOTE: each call to this method increments the connection counter!...
pfodMAC::challengeHashByteSize
static const uint8_t challengeHashByteSize
Definition: pfodMAC.h:90
pfodMAC::isBigEndian
boolean isBigEndian()
pfodMAC::initHash
void initHash()
pfodMAC::eeprom_read
uint8_t eeprom_read(int address)
pfodMAC::PowerCyclesOffset
static const uint8_t PowerCyclesOffset
Definition: pfodMAC.h:92
pfodMAC::noEEPROM
void noEEPROM()
pfodMAC::init
boolean init(int eepromAddress)
pfodMAC::eeprom_write
static void eeprom_write(int address, uint8_t value)
pfodMAC::pfodMAC
pfodMAC()
pfodMAC::readSecretKey
unsigned int readSecretKey(byte *bRtn, int keyAdd)
pfodMAC::checkMsgHash
boolean checkMsgHash(const byte *msgHash, uint16_t len)
Converts msgHash from hex Digits to bytes and then compares the resulting byte[] with the current has...
pfodMAC::getHashedResult
byte * getHashedResult()
pfodMAC::maxKeySize
static const uint8_t maxKeySize
Definition: pfodMAC.h:94
pfodMAC::finishHash
void finishHash()
pfodMAC::setDebugStream
void setDebugStream(Print *out)
pfodMAC::challengeByteSize
static const uint8_t challengeByteSize
Definition: pfodMAC.h:91
pfodMAC::msgHashByteSize
static const uint8_t msgHashByteSize
Definition: pfodMAC.h:89
pfodMAC::isValid
boolean isValid()
pfodMAC::resetPowerCycles
static void resetPowerCycles(int eepromAddress=0)
Use this call to reset the power cycles to 0xffff Then remove the call from the code for normal opera...
pfodMAC::printBytesInHex
void printBytesInHex(Print *out, const byte *b, size_t len)
pfodMAC::putLongToHash
void putLongToHash(uint32_t l)
pfodMAC::KeyOffset
static const uint8_t KeyOffset
Definition: pfodMAC.h:93
pfodMAC::setSecretKey
void setSecretKey(byte *key, int len)
pfodMAC::reverseBytes
void reverseBytes(byte *b, int len)
pfodMAC::putBytesToHash
void putBytesToHash(byte *b, int len)
pfodMAC::putByteToHash
void putByteToHash(byte b)
pfodEEPROM.h
pfodStream.h