| LIN_slave_portable_Arduino 1.4 Arduino library for Local Interconnect Network slave node emulation

Loading...
Searching...
No Matches
Public Attributes | List of all members
LIN_Slave_Base::callback_t Struct Reference

User-defined callback function with data length. More...

`#include <LIN_slave_Base.h>`

## Public Attributes
uint8_t | type_numData
| frame type (high nibble) and number of data bytes (low nibble)
LinMessageCallback | fct
| frame callback function

## Detailed Description

User-defined callback function with data length.

Definition at line 161 of file LIN_slave_Base.h.

## Member Data Documentation

## ◆ fct

LinMessageCallback LIN_Slave_Base::callback_t::fct

frame callback function

Definition at line 164 of file LIN_slave_Base.h.

## ◆ type_numData

uint8_t LIN_Slave_Base::callback_t::type_numData

frame type (high nibble) and number of data bytes (low nibble)

Definition at line 163 of file LIN_slave_Base.h.

The documentation for this struct was generated from the following file:

- LIN_slave_Base.h