# Default sdkconfig overrides for the esp-idf-pio build-validation example.
# PlatformIO merges this into the generated sdkconfig on every build.

# PsychicHttp requires WebSocket support in esp_http_server.
CONFIG_HTTPD_WS_SUPPORT=y

# Enable ESP-IDF HTTPS server (required by PsychicHttpsServer.h).
CONFIG_ESP_HTTPS_SERVER_ENABLE=y

# Ensure software mbedTLS MD5 implementation is compiled (not ROM-only).
# PsychicHttp calls mbedtls_md5_* directly for digest auth.
# CONFIG_MBEDTLS_ROM_MD5 is not set
