# Temperature

## Chips supported by ESensors

- [DS18x20](../chips/ds18x20.md)

- [DS3231](../chips/ds3231.md)

- [DHT22](../chips/dht.md)

- [STS4x](../chips/sts4x.md) with 0.2C accuracy


## Other chips

- [Testing Various Low-Cost Thermometers](https://www.kandrsmith.org/RJS/Misc/thermometers.html)

- [TMP117](https://www.bluedot.space/products/tmp117/): 0.1C accuracy.

- [TMP119](https://www.ti.com/product/TMP119): 0.08C accuracy.

- [TMP112](https://www.ti.com/product/TMP112): 0.5C accuracy.

- [MAX30205](https://www.analog.com/media/en/technical-documentation/data-sheets/max30205.pdf): 0.1C accuracy.

- [LM75A](https://www.ti.com/product/LM75A): 2C accuracy.

Modern, small temperature ICs:

- [TI TMP119](https://www.ti.com/product/TMP119) with
  0.08C accuracy in DSBGA package. [datasheet](../chips/datasheets/tmp119.pdf)

![TMP119](https://www.ti.com/ods/images/SNIS236/GUID-49797EB3-7BB6-48B9-8614-2688A39788BD-low.svg)

This chip is amazing.

Alternatives:

- [TI TMP112](https://www.ti.com/product/TMP112) with
  0.5C accuracy (SOT563 or X2SON).

![TMP112](https://www.ti.com/ods/images/SBOS473L/GUID-25E48344-B173-45DF-8E4F-51A8F8CB7C71-low.gif)

