SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

oled_ssd1306.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2017-2019, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
29 #ifndef _OLED_SSD1306_H_
30 #define _OLED_SSD1306_H_
31
32 #include "ssd1306_hal/io.h"
33
34 #ifdef __cplusplus
35 extern "C" {
36 #endif
37
51 void ssd1306_128x64_init(void);
52
61 void ssd1306_128x64_i2c_init(void);
62
78 void ssd1306_128x64_i2c_initEx(int8_t scl, int8_t sda, int8_t sa);
79
88 void ssd1306_128x64_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
89
98 void ssd1306_128x32_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
99
104 void ssd1306_init(void) __attribute__((deprecated));
105
114 void ssd1306_128x32_i2c_init(void);
115
124 void ssd1306_128x32_init(void);
125
129 void ssd1306_displayOff(void);
130
134 void ssd1306_displayOn(void);
135
140 void ssd1306_setContrast(uint8_t contrast);
141
147 void ssd1306_invertMode(void);
148
153 void ssd1306_normalMode(void);
154
164 void ssd1306_flipHorizontal(uint8_t mode);
165
175 void ssd1306_flipVertical(uint8_t mode);
176
182 void ssd1306_setStartLine(uint8_t line);
183
187 uint8_t ssd1306_getStartLine(void);
188
193 #ifdef __cplusplus
194 }
195 #endif
196
197 // ----------------------------------------------------------------------------
198 #endif // _OLED_SSD1306_H_
ssd1306_getStartLine
uint8_t ssd1306_getStartLine(void)
Definition: oled_ssd1306.c:164
ssd1306_flipVertical
void ssd1306_flipVertical(uint8_t mode)
performs vertical flip
Definition: oled_ssd1306.c:153
ssd1306_invertMode
void ssd1306_invertMode(void)
Definition: oled_ssd1306.c:138
ssd1306_setContrast
void ssd1306_setContrast(uint8_t contrast)
Definition: oled_ssd1306.c:130
ssd1306_128x32_init
void ssd1306_128x32_init(void)
Inits 128x32 OLED display (based on ssd1306 controller).
Definition: oled_ssd1306.c:225
ssd1306_128x64_spi_init
void ssd1306_128x64_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x64 OLED display over spi (based on SSD1306 controller).
Definition: oled_ssd1306.c:211
ssd1306_displayOff
void ssd1306_displayOff(void)
Definition: oled_ssd1306.c:119
ssd1306_flipHorizontal
void ssd1306_flipHorizontal(uint8_t mode)
performs horizontal flip
Definition: oled_ssd1306.c:148
io.h
ssd1306_128x64_init
void ssd1306_128x64_init(void)
Inits 128x64 OLED display (based on SSD1306 controller).
Definition: oled_ssd1306.c:179
ssd1306_128x64_i2c_initEx
void ssd1306_128x64_i2c_initEx(int8_t scl, int8_t sda, int8_t sa)
Inits 128x64 OLED display over i2c (based on SSD1306 controller).
Definition: oled_ssd1306.c:201
ssd1306_128x32_i2c_init
void ssd1306_128x32_i2c_init(void)
Inits 128x32 OLED display over i2c (based on SSD1306 controller).
Definition: oled_ssd1306.c:241
ssd1306_128x64_i2c_init
void ssd1306_128x64_i2c_init(void)
Inits 128x64 OLED display over i2c (based on SSD1306 controller).
Definition: oled_ssd1306.c:195
ssd1306_displayOn
void ssd1306_displayOn(void)
Definition: oled_ssd1306.c:125
ssd1306_setStartLine
void ssd1306_setStartLine(uint8_t line)
Definition: oled_ssd1306.c:158
ssd1306_128x32_spi_init
void ssd1306_128x32_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x32 OLED display over spi (based on SSD1306 controller).
Definition: oled_ssd1306.c:251
ssd1306_normalMode
void ssd1306_normalMode(void)
Definition: oled_ssd1306.c:143
ssd1306_init
void ssd1306_init(void) __attribute__((deprecated))
Inits 128x64 OLED display over i2c (based on SSD1306 controller).
Definition: oled_ssd1306.c:173