SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Public Member Functions | List of all members
NanoCanvas16 Class Reference

`#include <canvas.h>`

Inheritance diagram for NanoCanvas16:

## Public Member Functions
void | blt (lcdint_t x, lcdint_t y) override
void | blt () override
void | blt (const NanoRect &rect) override
Public Member Functions inherited from NanoCanvasOps< BPP >
| NanoCanvasOps ()
| NanoCanvasOps (lcdint_t w, lcdint_t h, uint8_t *bytes)
void | begin (lcdint_t w, lcdint_t h, uint8_t *bytes)
void | setOffset (lcdint_t ox, lcdint_t oy)
const NanoPoint | offsetEnd () const
const NanoRect | rect () const
void | putPixel (lcdint_t x, lcdint_t y)
void | putPixel (const NanoPoint &p)
void | drawVLine (lcdint_t x1, lcdint_t y1, lcdint_t y2)
void | drawHLine (lcdint_t x1, lcdint_t y1, lcdint_t x2)
void | drawLine (lcdint_t x1, lcdint_t y1, lcdint_t x2, lcdint_t y2)
void | drawLine (const NanoRect &rect)
void | drawRect (lcdint_t x1, lcdint_t y1, lcdint_t x2, lcdint_t y2)
void | drawRect (const NanoRect &rect)
void | fillRect (lcdint_t x1, lcdint_t y1, lcdint_t x2, lcdint_t y2)
void | fillRect (const NanoRect &rect)
void | drawBitmap1 (lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *bitmap)
| Draws monochrome bitmap in color buffer using color, specified via setColor() method Draws monochrome bitmap in color buffer using color, specified via setColor() method The bitmap is expected in Native ssd1306 controller format. More...
void | drawXBitmap1 (lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *bitmap)
| Draws monochrome bitmap in color buffer using color, specified via setColor() method Draws monochrome bitmap in color buffer using color, specified via setColor() method The bitmap is expected in XBMP format. More...
void | drawBitmap8 (lcdint_t x, lcdint_t y, lcduint_t w, lcduint_t h, const uint8_t *bitmap)
| Draws 8-bit color bitmap in color buffer. Draws 8-bit color bitmap in color buffer. More...
void | clear ()
size_t | write (uint8_t c) override
uint8_t | printChar (uint8_t c)
void | printFixed (lcdint_t xpos, lcdint_t y, const char *ch, EFontStyle style=STYLE_NORMAL)
void | printFixedPgm (lcdint_t xpos, lcdint_t y, const char *ch, EFontStyle style=STYLE_NORMAL)
void | setMode (uint8_t modeFlags)
| Sets canvas drawing mode Sets canvas drawing mode. The set flags define transparency of output images. More...
void | setColor (uint16_t color)
Public Member Functions inherited from Print
| Print ()
size_t | print (const char *str)
size_t | print (int n)
size_t | println (const char *str)
size_t | println (int data)

## Additional Inherited Members
Public Attributes inherited from NanoCanvasOps< BPP >
NanoPoint | offset = { 0, 0 }
Static Public Attributes inherited from NanoCanvasOps< BPP >
static const uint8_t | BITS_PER_PIXEL = BPP
Protected Attributes inherited from NanoCanvasOps< BPP >
lcduint_t | m_w
| width of NanoCanvas area in pixels
lcduint_t | m_h
| height of NanoCanvas area in pixels
lcduint_t | m_p
| number of bits, used by width value: 3 equals to 8 pixels width
lcdint_t | m_cursorX
| current X cursor position for text output
lcdint_t | m_cursorY
| current Y cursor position for text output
uint8_t | m_textMode
| Flags for current NanoCanvas mode.
EFontStyle | m_fontStyle
| currently active font style
uint8_t * | m_buf
| Canvas data.
uint16_t | m_color
| current color for monochrome operations

## Detailed Description

NanoCanvas16 represents objects for drawing in memory buffer NanoCanvas16 represents each pixel as 2-bytes with RGB bits: RRRRRGGG-GGGBBBBB For details refer to SSD1351 datasheet

Definition at line 577 of file canvas.h.

## Member Function Documentation

## ◆ blt() [1/3]

void NanoCanvas16::blt | ( | lcdint_t | x,
|  | lcdint_t | y
| ) |  |
| override virtual

Draws canvas on the LCD display

Parameters

  x | - horizontal position in pixels
  y | - vertical position in pixels

Implements NanoCanvasBase< 16 >.

## ◆ blt() [2/3]

void NanoCanvas16::blt | ( |  | ) |
| override virtual

Draws canvas on the LCD display using offset values.

Implements NanoCanvasBase< 16 >.

## ◆ blt() [3/3]

void NanoCanvas16::blt | ( | const NanoRect & | rect | ) |
| override virtual

Draws only part of canvas on the LCD display. This method uses Canvas offset field as top-left point of whole canvas content. First point of specified rectangle defines the actual top-left point on the screen to be refreshed. For example, `blt({{8,0},{15,7}});` will copy canvas area {8,0}-{15,7} to screen starting at {8,0} if canvas offset is {0,0}. If canvas offset is {12,3}, then canvas area {8,0}-{15,7} will be copied to screen at position {20,3}.

Parameters

  rect | rectagle describing part of canvas to move to display.

Implements NanoCanvasBase< 16 >.

The documentation for this class was generated from the following file:

- nano_engine/canvas.h