\doxysection{src/\+Me\+On\+Board\+Temp.cpp File Reference}
\hypertarget{_me_on_board_temp_8cpp}{}\label{_me_on_board_temp_8cpp}\index{src/MeOnBoardTemp.cpp@{src/MeOnBoardTemp.cpp}}


Driver for Auriga On Board Temperature device.  


{\ttfamily \#include "{}Me\+On\+Board\+Temp.\+h"{}}\newline
Include dependency graph for Me\+On\+Board\+Temp.\+cpp\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_on_board_temp_8cpp__incl}
\end{center}
\end{figure}
\doxysubsubsection*{Variables}
\begin{DoxyCompactItemize}
\item 
\Hypertarget{_me_on_board_temp_8cpp_a621dc3f6cd950f046439aeb59928ef63}\label{_me_on_board_temp_8cpp_a621dc3f6cd950f046439aeb59928ef63} 
const int16\+\_\+t {\bfseries TEMPERATURENOMINAL} = 25
\item 
\Hypertarget{_me_on_board_temp_8cpp_a9fa348aa098acd9f86fb076bb31fdb3f}\label{_me_on_board_temp_8cpp_a9fa348aa098acd9f86fb076bb31fdb3f} 
const int16\+\_\+t {\bfseries SERIESRESISTOR} = 10000
\item 
\Hypertarget{_me_on_board_temp_8cpp_a0e982e56c6272b902fbcac5bc3ec15da}\label{_me_on_board_temp_8cpp_a0e982e56c6272b902fbcac5bc3ec15da} 
const int16\+\_\+t {\bfseries BCOEFFICIENT} = 3380
\item 
\Hypertarget{_me_on_board_temp_8cpp_af73a0c946d825b18b3424f696cab2cb7}\label{_me_on_board_temp_8cpp_af73a0c946d825b18b3424f696cab2cb7} 
const int16\+\_\+t {\bfseries TERMISTORNOMINAL} = 10000
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Driver for Auriga On Board Temperature device. 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+0 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2016/04/01 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2016, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V2 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V2}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 2 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
This file is a drive for On Board Temperature device.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\end{DoxyParagraph}

\begin{DoxyEnumerate}
\item void Me\+On\+Board\+Temp\+::setpin(uint8\+\_\+t digital\+\_\+pin,uint8\+\_\+t analog\+\_\+pin);
\item int16\+\_\+t \doxylink{class_me_on_board_temp_ada9bb788ed99094df48dbd9536193362}{Me\+On\+Board\+Temp\+::read\+Analog(void)}
\item float \doxylink{class_me_on_board_temp_a590a42d0aab644a6c7108d3f47b477b3}{Me\+On\+Board\+Temp\+::read\+Value(void)};
\end{DoxyEnumerate}

\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Mark Yan         2016/04/01     1.0.0            build the new.
\end{DoxyPre}
 
\end{DoxyParagraph}
